(footprint "TO-263-2"
	(version 20240108)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "TO-263/D2PAK/DDPAK SMD package, http://www.infineon.com/cms/en/product/packages/PG-TO263/PG-TO263-3-1/")
	(tags "D2PAK DDPAK TO-263 D2PAK-3 TO-263-3 SOT-404")
	(property "Reference" "REF**"
		(at 0 -6.65 0)
		(layer "F.SilkS")
	)
	(property "Value" "TO-263-2"
		(at 0 6.65 0)
		(layer "F.Fab")
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -7.65 -2.54)
		(size 4.6 1.1)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.227273)
	)
	(pad "2" smd roundrect
		(at -0.925 -2.775)
		(size 4.55 5.25)
		(layers "F.Cu" "F.Paste")
		(roundrect_rratio 0.054945)
	)
	(pad "2" smd roundrect
		(at -0.925 2.775)
		(size 4.55 5.25)
		(layers "F.Cu" "F.Paste")
		(roundrect_rratio 0.054945)
	)
	(pad "2" smd roundrect
		(at 1.5 0)
		(size 9.4 10.8)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.026596)
	)
	(pad "2" smd roundrect
		(at 3.925 -2.775)
		(size 4.55 5.25)
		(layers "F.Cu" "F.Paste")
		(roundrect_rratio 0.054945)
	)
	(pad "2" smd roundrect
		(at 3.925 2.775)
		(size 4.55 5.25)
		(layers "F.Cu" "F.Paste")
		(roundrect_rratio 0.054945)
	)
	(pad "3" smd roundrect
		(at -7.65 2.54)
		(size 4.6 1.1)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.227273)
	)
	(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/TO-263-2.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
