(footprint "TO-263-9_TabPin10"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "TO-263 / D2PAK / DDPAK SMD package, http://www.ti.com/lit/ds/symlink/lm4755.pdf")
	(tags "D2PAK DDPAK TO-263 D2PAK-9 TO-263-9")
	(property "Reference" "REF**"
		(at -1.875 -6.65 0)
		(layer "F.SilkS")
	)
	(property "Value" "TO-263-9_TabPin10"
		(at -1.875 6.65 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at -1.875 0 0)
		(layer "F.Fab")
	)
	(pad "" smd roundrect
		(at -0.925 -2.775)
		(size 4.55 5.25)
		(layers "F.Paste")
		(roundrect_rratio 0.05494505495)
	)
	(pad "" smd roundrect
		(at -0.925 2.775)
		(size 4.55 5.25)
		(layers "F.Paste")
		(roundrect_rratio 0.05494505495)
	)
	(pad "" smd roundrect
		(at 3.925 -2.775)
		(size 4.55 5.25)
		(layers "F.Paste")
		(roundrect_rratio 0.05494505495)
	)
	(pad "" smd roundrect
		(at 3.925 2.775)
		(size 4.55 5.25)
		(layers "F.Paste")
		(roundrect_rratio 0.05494505495)
	)
	(pad "1" smd roundrect
		(at -7.65 -3.88)
		(size 4.6 0.61)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "2" smd roundrect
		(at -7.65 -2.91)
		(size 4.6 0.61)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "3" smd roundrect
		(at -7.65 -1.94)
		(size 4.6 0.61)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "4" smd roundrect
		(at -7.65 -0.97)
		(size 4.6 0.61)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "5" smd roundrect
		(at -7.65 0)
		(size 4.6 0.61)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "6" smd roundrect
		(at -7.65 0.97)
		(size 4.6 0.61)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "7" smd roundrect
		(at -7.65 1.94)
		(size 4.6 0.61)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "8" smd roundrect
		(at -7.65 2.91)
		(size 4.6 0.61)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "9" smd roundrect
		(at -7.65 3.88)
		(size 4.6 0.61)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "10" smd roundrect
		(at 1.5 0)
		(size 9.4 10.8)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.02659574468)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/TO-263-9_TabPin10.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
