(footprint "TO-268-2"
	(version 20240108)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "TO-268/D3PAK SMD package, http://www.icbank.com/icbank_data/semi_package/to268aa_dim.pdf")
	(tags "D3PAK TO-268 D3PAK-3 TO-268-3")
	(property "Reference" "REF**"
		(at 0 -9.55 0)
		(layer "F.SilkS")
	)
	(property "Value" "TO-268-2"
		(at 0 9.55 0)
		(layer "F.Fab")
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -9.975 -5.45)
		(size 5 3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.083333)
	)
	(pad "2" smd roundrect
		(at -0.725 -4.225)
		(size 6.6 8.15)
		(layers "F.Cu" "F.Paste")
		(roundrect_rratio 0.037879)
	)
	(pad "2" smd roundrect
		(at -0.725 4.225)
		(size 6.6 8.15)
		(layers "F.Cu" "F.Paste")
		(roundrect_rratio 0.037879)
	)
	(pad "2" smd roundrect
		(at 2.725 0)
		(size 13.5 16.6)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.018519)
	)
	(pad "2" smd roundrect
		(at 6.175 -4.225)
		(size 6.6 8.15)
		(layers "F.Cu" "F.Paste")
		(roundrect_rratio 0.037879)
	)
	(pad "2" smd roundrect
		(at 6.175 4.225)
		(size 6.6 8.15)
		(layers "F.Cu" "F.Paste")
		(roundrect_rratio 0.037879)
	)
	(pad "3" smd roundrect
		(at -9.975 5.45)
		(size 5 3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.083333)
	)
	(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/TO-268-2.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
