(footprint "TO-50-4_ShortPad-NoHole_Housing"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "TO-50-4 Macro X Package Style M238")
	(tags "TO-50-4 Macro X Package Style M238")
	(property "Reference" "REF**"
		(at 3.93 -3.87 0)
		(layer "F.SilkS")
	)
	(property "Value" "TO-50-4_ShortPad-NoHole_Housing"
		(at 15.32 4.68 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0.375 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -5.6 0 270)
		(size 1.5 4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -0.4 5.2 270)
		(size 4 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at 5.6 0 270)
		(size 1.5 5.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -0.4 -5.2 270)
		(size 4 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/TO-50-4_ShortPad-NoHole_Housing.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
