(footprint "Texas_NDQ"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Texas Instruments, NDQ, 5 pin (https://www.ti.com/lit/ml/mmsf022/mmsf022.pdf)")
	(tags "ti pfm dap")
	(property "Reference" "REF**"
		(at 0.2025 -6 0)
		(layer "F.SilkS")
	)
	(property "Value" "Texas_NDQ"
		(at 0.2025 6 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0.2025 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -8.315 -3.4)
		(size 2.41 1.07)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "2" smd roundrect
		(at -8.315 -1.7)
		(size 2.41 1.07)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "3" smd roundrect
		(at -8.315 0)
		(size 2.41 1.07)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "4" smd roundrect
		(at -8.315 1.7)
		(size 2.41 1.07)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "5" smd roundrect
		(at -8.315 3.4)
		(size 2.41 1.07)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "6" smd roundrect
		(at 0.91 0)
		(size 6.35 5.59)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.04472271914)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/Texas_NDQ.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
