(footprint "Texas_NDY0011A"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "TO-PMOD-11 11-pin switching regulator package, http://www.ti.com/lit/ml/mmsf025/mmsf025.pdf")
	(tags "Texas TO-PMOD NDY00011A")
	(property "Reference" "REF**"
		(at 8.5 0 270)
		(layer "F.SilkS")
	)
	(property "Value" "Texas_NDY0011A"
		(at -12 0 270)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 270)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -9.5 -6.35 270)
		(size 0.86 2.41)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "2" smd roundrect
		(at -9.5 -5.08 270)
		(size 0.86 2.41)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "3" smd roundrect
		(at -9.5 -3.81 270)
		(size 0.86 2.41)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "4" smd roundrect
		(at -9.5 -2.54 270)
		(size 0.86 2.41)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "5" smd roundrect
		(at -9.5 -1.27 270)
		(size 0.86 2.41)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "6" smd roundrect
		(at -9.5 0 270)
		(size 0.86 2.41)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "7" smd roundrect
		(at -9.5 1.27 270)
		(size 0.86 2.41)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "8" smd roundrect
		(at -9.5 2.54 270)
		(size 0.86 2.41)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "9" smd roundrect
		(at -9.5 3.81 270)
		(size 0.86 2.41)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "10" smd roundrect
		(at -9.5 5.08 270)
		(size 0.86 2.41)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "11" smd roundrect
		(at -9.5 6.35 270)
		(size 0.86 2.41)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "12" smd roundrect
		(at 0 0 270)
		(size 9.126 13.37)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.02739425816)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/Texas_NDY0011A.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
