(footprint "Vishay_PowerPAK_SC70-6L_Single"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Vishay PowerPAK SC70 single transistor package http://www.vishay.com/docs/70486/70486.pdf")
	(tags "powerpak sc70 sc-70")
	(property "Reference" "REF**"
		(at 0 -2 0)
		(layer "F.SilkS")
	)
	(property "Value" "Vishay_PowerPAK_SC70-6L_Single"
		(at 0 2 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" smd roundrect
		(at -0.35 -0.325)
		(size 0.6 0.8)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 0.35 -0.325)
		(size 0.6 0.8)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "1" smd custom
		(at 0 -0.325)
		(size 1.5 0.95)
		(layers "F.Cu" "F.Mask")
		(zone_connect 2)
		(thermal_bridge_angle 45)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy 1.1 -0.175) (xy -1.1 -0.175) (xy -1.1 -0.475) (xy 1.1 -0.475)
				)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 1.1 0.475) (xy -1.1 0.475) (xy -1.1 0.175) (xy 1.1 0.175)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "3" smd roundrect
		(at -0.925 0.65)
		(size 0.35 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "4" smd roundrect
		(at 0.04 0.65)
		(size 0.87 0.235)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "4" smd roundrect
		(at 0.925 0.65)
		(size 0.35 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/Vishay_PowerPAK_SC70-6L_Single.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
