(footprint "Analog_TO-46-4_ThermalShield"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "TO-46-4 with Valox case, based on https://www.analog.com/media/en/technical-documentation/data-sheets/199399fc.pdf")
	(tags "TO-46-4 LM399")
	(property "Reference" "REF**"
		(at 2.032 -6.477 0)
		(layer "F.SilkS")
	)
	(property "Value" "Analog_TO-46-4_ThermalShield"
		(at 1.27 3.556 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "REF**"
		(at 2.032 -6.477 0)
		(layer "F.Fab")
	)
	(fp_text user "${REFERENCE}"
		(at 1.25 0 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole oval
		(at 0 0)
		(size 1.6 1.2)
		(drill 0.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 1.27 1.27)
		(size 1.2 1.2)
		(drill 0.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at 2.54 0)
		(size 1.2 1.2)
		(drill 0.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 1.27 -1.27)
		(size 1.2 1.2)
		(drill 0.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/Analog_TO-46-4_ThermalShield.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
