(footprint "SOT-227"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "SOT-227 / SOT-227B / ISOTOP, M4 mounting screws (https://www.vishay.com/docs/95423/sot227g2.pdf, https://www.vishay.com/docs/95793/vs-fc420sa10.pdf)")
	(tags "sot 227 isotop")
	(property "Reference" "REF**"
		(at 7.525 -7.125 0)
		(layer "F.SilkS")
	)
	(property "Value" "SOT-227"
		(at 7.525 7.375 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 7.525 5.375 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at 0 -0.665)
		(size 8.55 10.88)
		(layers "F.Cu" "F.Mask")
	)
	(pad "1" thru_hole circle
		(at 0 0)
		(size 8 8)
		(drill 4.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" smd rect
		(at 15.05 -0.665)
		(size 8.55 10.88)
		(layers "F.Cu" "F.Mask")
	)
	(pad "2" thru_hole circle
		(at 15.05 0)
		(size 8 8)
		(drill 4.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at 15.05 12.75)
		(size 8 8)
		(drill 4.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" smd rect
		(at 15.05 13.415)
		(size 8.55 10.88)
		(layers "F.Cu" "F.Mask")
	)
	(pad "4" thru_hole circle
		(at 0 12.75)
		(size 8 8)
		(drill 4.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" smd rect
		(at 0 13.415)
		(size 8.55 10.88)
		(layers "F.Cu" "F.Mask")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/SOT-227.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
