(footprint "TO-126-3_Horizontal_TabDown"
	(version 20240108)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "TO-126-3, Horizontal, RM 2.28mm, see https://www.diodes.com/assets/Package-Files/TO126.pdf")
	(tags "TO-126-3 Horizontal RM 2.28mm")
	(property "Reference" "REF**"
		(at 2.28 -16.12 0)
		(layer "F.SilkS")
	)
	(property "Value" "TO-126-3_Horizontal_TabDown"
		(at 2.28 1.9 0)
		(layer "F.Fab")
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 2.28 -16.12 0)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at 2.28 -11.1)
		(size 3.2 3.2)
		(drill 3.2)
		(layers "*.Cu" "*.Mask")
	)
	(pad "1" thru_hole rect
		(at 0 0)
		(size 1.71 1.8)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole oval
		(at 2.28 0)
		(size 1.71 1.8)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole oval
		(at 4.56 0)
		(size 1.71 1.8)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-126-3_Horizontal_TabDown.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
