(footprint "TO-218-2_Vertical"
	(version 20240108)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "TO-218-2, Vertical, RM 10.95mm, SOT-93, see https://www.vishay.com/docs/95214/fto218.pdf")
	(tags "TO-218-2 Vertical RM 10.95mm SOT-93")
	(property "Reference" "REF**"
		(at 5.475 -4.29 0)
		(layer "F.SilkS")
	)
	(property "Value" "TO-218-2_Vertical"
		(at 5.475 3 0)
		(layer "F.Fab")
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 5.475 -4.29 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole rect
		(at 0 0)
		(size 2.5 3.5)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole oval
		(at 10.95 0)
		(size 2.5 3.5)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-218-2_Vertical.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
