(footprint "TO-251-2_Vertical"
	(version 20240108)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "TO-251-2, Vertical, RM 4.58mm, IPAK, see https://www.diodes.com/assets/Package-Files/TO251.pdf")
	(tags "TO-251-2 Vertical RM 4.58mm IPAK")
	(property "Reference" "REF**"
		(at 2.29 -2.39 0)
		(layer "F.SilkS")
	)
	(property "Value" "TO-251-2_Vertical"
		(at 2.29 2.28 0)
		(layer "F.Fab")
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 2.29 -2.39 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole rect
		(at 0 0)
		(size 1.8 1.8)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 4.58 0)
		(size 1.8 1.8)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-251-2_Vertical.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
