(footprint "TO-251-3-1EP_Horizontal_TabDown"
	(version 20240108)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "TO-251-3, Horizontal, RM 2.29mm, IPAK, see https://www.diodes.com/assets/Package-Files/TO251.pdf")
	(tags "TO-251-3 Horizontal RM 2.29mm IPAK")
	(property "Reference" "REF**"
		(at 2.29 -11.653333 0)
		(layer "F.SilkS")
	)
	(property "Value" "TO-251-3-1EP_Horizontal_TabDown"
		(at 2.29 1.9 0)
		(layer "F.Fab")
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 2.29 -11.653333 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole rect
		(at 0 0)
		(size 1.7175 1.8)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole oval
		(at 2.29 0)
		(size 1.7175 1.8)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole oval
		(at 4.58 0)
		(size 1.7175 1.8)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" smd rect
		(at 2.29 -7.433333)
		(size 5.7 6.2)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-251-3-1EP_Horizontal_TabDown.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
