(footprint "TO-262-3-1EP_Horizontal_TabDown"
	(version 20240108)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "TO-262-3, Horizontal, RM 2.54mm, IIPAK, I2PAK, see http://www.onsemi.com/pub/Collateral/EN8586-D.PDF")
	(tags "TO-262-3 Horizontal RM 2.54mm IIPAK I2PAK")
	(property "Reference" "REF**"
		(at 2.54 -16.103333 0)
		(layer "F.SilkS")
	)
	(property "Value" "TO-262-3-1EP_Horizontal_TabDown"
		(at 2.54 2 0)
		(layer "F.Fab")
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 2.54 -16.103333 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole rect
		(at 0 0)
		(size 1.905 2)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole oval
		(at 2.54 0)
		(size 1.905 2)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole oval
		(at 5.08 0)
		(size 1.905 2)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" smd rect
		(at 2.54 -10.983333)
		(size 10 8)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-262-3-1EP_Horizontal_TabDown.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
