(footprint "TO-264-3_Vertical"
	(version 20240108)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "TO-264-3, Vertical, RM 5.45mm, see https://www.fairchildsemi.com/package-drawings/TO/TO264A03.pdf")
	(tags "TO-264-3 Vertical RM 5.45mm")
	(property "Reference" "REF**"
		(at 5.45 -3.02 0)
		(layer "F.SilkS")
	)
	(property "Value" "TO-264-3_Vertical"
		(at 5.45 4.35 0)
		(layer "F.Fab")
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 5.45 -3.02 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole rect
		(at 0 0)
		(size 2.5 4.5)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole oval
		(at 5.45 0)
		(size 2.5 4.5)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole oval
		(at 10.9 0)
		(size 2.5 4.5)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-264-3_Vertical.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
