(footprint "TO-264-5_Horizontal_TabUp"
	(version 20240108)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "TO-264-5, Horizontal, RM 3.81mm, see https://www.onsemi.com/pub/Collateral/NJL3281D-D.PDF")
	(tags "TO-264-5 Horizontal RM 3.81mm")
	(property "Reference" "REF**"
		(at 7.62 32.2 0)
		(layer "F.SilkS")
	)
	(property "Value" "TO-264-5_Horizontal_TabUp"
		(at 7.62 -3.25 0)
		(layer "F.Fab")
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 7.62 32.2 0)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at 7.62 25.08)
		(size 3.3 3.3)
		(drill 3.3)
		(layers "*.Cu" "*.Mask")
	)
	(pad "1" thru_hole rect
		(at 0 0)
		(size 2.5 4.5)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole oval
		(at 3.81 0)
		(size 2.5 4.5)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole oval
		(at 7.62 0)
		(size 2.5 4.5)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole oval
		(at 11.43 0)
		(size 2.5 4.5)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole oval
		(at 15.24 0)
		(size 2.5 4.5)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-264-5_Horizontal_TabUp.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
