(footprint "TO-92L_HandSolder"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "TO-92L leads in-line (large body variant of TO-92), also known as TO-226, wide, drill 0.75mm, hand-soldering variant with enlarged pads (see https://www.diodes.com/assets/Package-Files/TO92L.pdf and http://www.ti.com/lit/an/snoa059/snoa059.pdf)")
	(tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
	(property "Reference" "REF**"
		(at 1.27 -3.8 0)
		(layer "F.SilkS")
	)
	(property "Value" "TO-92L_HandSolder"
		(at 1.27 2.79 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 1.27 0 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole rect
		(at 0 0)
		(size 1.1 1.8)
		(drill 0.75
			(offset 0 0.4)
		)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole roundrect
		(at 1.27 -1.27)
		(size 1.1 1.8)
		(drill 0.75
			(offset 0 -0.4)
		)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.25)
	)
	(pad "3" thru_hole roundrect
		(at 2.54 0)
		(size 1.1 1.8)
		(drill 0.75
			(offset 0 0.4)
		)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.25)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-92L.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
