(footprint "Potentiometer_ACP_CA6-VSMD_Vertical"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Potentiometer, vertical, ACP CA6-VSMD, http://www.acptechnologies.com/wp-content/uploads/2017/06/01-ACP-CA6.pdf")
	(tags "Potentiometer vertical ACP CA6-VSMD")
	(property "Reference" "REF**"
		(at 0 -4.5 0)
		(layer "F.SilkS")
	)
	(property "Value" "Potentiometer_ACP_CA6-VSMD_Vertical"
		(at 0 4.5 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at -2.25 0 90)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -4.325 2.15)
		(size 2.5 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at 4.325 0)
		(size 2.5 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -4.325 -2.15)
		(size 2.5 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Potentiometer_SMD.3dshapes/Potentiometer_ACP_CA6-VSMD_Vertical.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
