(footprint "Potentiometer_ACP_CA9-VSMD_Vertical_Hole"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Potentiometer, vertical, shaft hole, ACP CA9-VSMD, http://www.acptechnologies.com/wp-content/uploads/2017/05/02-ACP-CA9-CE9.pdf")
	(tags "Potentiometer vertical hole ACP CA9-VSMD")
	(property "Reference" "REF**"
		(at 0 -6.15 0)
		(layer "F.SilkS")
	)
	(property "Value" "Potentiometer_ACP_CA9-VSMD_Vertical_Hole"
		(at 0 6.15 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at -4 0 90)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at 0.125 0)
		(size 4 4)
		(drill 4)
		(layers "*.Cu" "*.Mask")
	)
	(pad "1" smd rect
		(at -4.625 2.5)
		(size 2.5 2.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at 4.625 0)
		(size 2.5 2.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -4.625 -2.5)
		(size 2.5 2.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Potentiometer_SMD.3dshapes/Potentiometer_ACP_CA9-VSMD_Vertical_Hole.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
