(footprint "Potentiometer_Bourns_3314G_Vertical"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Potentiometer, vertical, top-adjust, Bourns 3314G, http://www.bourns.com/docs/Product-Datasheets/3314.pdf")
	(tags "Potentiometer vertical Bourns 3314G")
	(property "Reference" "REF**"
		(at 0 -4.65 0)
		(layer "F.SilkS")
	)
	(property "Value" "Potentiometer_Bourns_3314G_Vertical"
		(at 0 4.65 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 -1.7 0)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -1.15 -2.75)
		(size 1.3 1.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1923076923)
	)
	(pad "2" smd roundrect
		(at 0 2.75)
		(size 2 1.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1923076923)
	)
	(pad "3" smd roundrect
		(at 1.15 -2.75)
		(size 1.3 1.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1923076923)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Potentiometer_SMD.3dshapes/Potentiometer_Bourns_3314G_Vertical.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
