(footprint "Potentiometer_Bourns_3314S_Horizontal"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Potentiometer, horizontal, Bourns 3314S, http://www.bourns.com/docs/Product-Datasheets/3314.pdf")
	(tags "Potentiometer horizontal Bourns 3314S")
	(property "Reference" "REF**"
		(at 0 -4.15 0)
		(layer "F.SilkS")
	)
	(property "Value" "Potentiometer_Bourns_3314S_Horizontal"
		(at 0 4.15 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -1.15 -2.025)
		(size 1.2 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2083333333)
	)
	(pad "2" smd roundrect
		(at 0 2.025)
		(size 1.6 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15625)
	)
	(pad "3" smd roundrect
		(at 1.15 -2.025)
		(size 1.2 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2108333333)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Potentiometer_SMD.3dshapes/Potentiometer_Bourns_3314S_Horizontal.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
