(footprint "Potentiometer_Alpha_RD902F-40-00D_Dual_Vertical"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Potentiometer, vertical, 9mm, dual, http://www.taiwanalpha.com.tw/downloads?target=products&id=113")
	(tags "potentiometer vertical 9mm dual")
	(property "Reference" "REF**"
		(at 6.35 -5.06 180)
		(layer "F.SilkS")
	)
	(property "Value" "Potentiometer_Alpha_RD902F-40-00D_Dual_Vertical"
		(at 0 10.16 180)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 7.62 2.54 0)
		(layer "F.Fab")
	)
	(pad "" thru_hole oval
		(at 7.5 -2.25 90)
		(size 2.72 3.24)
		(drill oval 1.1 1.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "" thru_hole oval
		(at 7.5 7.25 90)
		(size 2.72 3.24)
		(drill oval 1.1 1.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole rect
		(at 0 0 90)
		(size 1.8 1.8)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 0 2.5 90)
		(size 1.8 1.8)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at 0 5 90)
		(size 1.8 1.8)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at -2.5 0 90)
		(size 1.8 1.8)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole circle
		(at -2.5 2.5 90)
		(size 1.8 1.8)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "6" thru_hole circle
		(at -2.5 5 90)
		(size 1.8 1.8)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Potentiometer_THT.3dshapes/Potentiometer_Alpha_RD902F-40-00D_Dual_Vertical.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
