(footprint "Potentiometer_Alps_RK09K_Single_Horizontal"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "111009J 1110AK4 11100DN 1110AAR 1110077 1110A0J 110AMJ 1110B26 D1110C1A Potentiometer, horizontal, Alps RK09K Single, https://tech.alpsalpine.com/prod/e/pdf/potentiometer/rotarypotentiometers/rk09k/rk09k.pdf")
	(tags "Potentiometer horizontal Alps RK09K Single Snapin")
	(property "Reference" "REF**"
		(at 0 11.05 180)
		(layer "F.SilkS")
	)
	(property "Value" "Potentiometer_Alps_RK09K_Single_Horizontal"
		(at 0 -6.05 180)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 0 2.5 180)
		(layer "F.Fab")
	)
	(pad "1" thru_hole rect
		(at 0 0 180)
		(size 1.8 1.8)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 0 2.5 180)
		(size 1.8 1.8)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at 0 5 180)
		(size 1.8 1.8)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "MP" thru_hole roundrect
		(at 3.3 -2.5 180)
		(size 4 3)
		(drill oval 2.1 1.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.25)
	)
	(pad "MP" thru_hole roundrect
		(at 3.3 7.5 180)
		(size 4 3)
		(drill oval 2.1 1.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.25)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(name "Copper Keep Out")
		(hatch full 0.508)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints not_allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy -2.75 -2.5) (xy -1.25 -2.5) (xy -1.25 -1.85) (xy -2.75 -1.85)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(name "Copper Keep Out")
		(hatch full 0.508)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints not_allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy -2.75 6.85) (xy -1.25 6.85) (xy -1.25 7.5) (xy -2.75 7.5)
			)
		)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Potentiometer_THT.3dshapes/Potentiometer_Alps_RK09K_Single_Horizontal.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
