(footprint "Potentiometer_Alps_RK09K_Single_Vertical"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "113004U 1130A6S 11300DR 1130A8G 1130081 1130A5R 1130AP5 1130AST  D1130C3W D1130C1B D1130C3C D1130C2P Potentiometer, vertical, Alps RK09K Single, https://tech.alpsalpine.com/prod/e/pdf/potentiometer/rotarypotentiometers/rk09k/rk09k.pdf")
	(tags "Potentiometer vertical Alps RK09K RK09D Single Snapin")
	(property "Reference" "REF**"
		(at 6.05 -5.15 0)
		(layer "F.SilkS")
	)
	(property "Value" "Potentiometer_Alps_RK09K_Single_Vertical"
		(at 6.05 10.15 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 2 2.5 90)
		(layer "F.Fab")
	)
	(pad "1" thru_hole rect
		(at 0 0)
		(size 1.8 1.8)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 0 2.5)
		(size 1.8 1.8)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at 0 5)
		(size 1.8 1.8)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "MP" thru_hole roundrect
		(at 7 -1.9)
		(size 4 3)
		(drill oval 2.1 1.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.25)
	)
	(pad "MP" thru_hole roundrect
		(at 7 6.9)
		(size 4 3)
		(drill oval 2.1 1.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.25)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Potentiometer_THT.3dshapes/Potentiometer_Alps_RK09K_Single_Vertical.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
