(footprint "Potentiometer_Alps_RK09L_Double_Horizontal"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "122002H 122002L 12B0A4S 12B0A1V Potentiometer, horizontal, Alps RK09L Double, https://tech.alpsalpine.com/prod/e/pdf/potentiometer/rotarypotentiometers/rk09l/rk09l.pdf")
	(tags "Potentiometer horizontal Alps RK09L Double")
	(property "Reference" "REF**"
		(at 0 10.6 180)
		(layer "F.SilkS")
	)
	(property "Value" "Potentiometer_Alps_RK09L_Double_Horizontal"
		(at 0 8.1 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at -0.43 2.5 180)
		(layer "F.Fab")
	)
	(pad "1" thru_hole rect
		(at 0 0 180)
		(size 1.8 1.8)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 0 2.5 180)
		(size 1.8 1.8)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at 0 5 180)
		(size 1.8 1.8)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 2.5 0 180)
		(size 1.8 1.8)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole circle
		(at 2.5 2.5 180)
		(size 1.8 1.8)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "6" thru_hole circle
		(at 2.5 5 180)
		(size 1.8 1.8)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "MP" thru_hole roundrect
		(at 5.8 -2.25 180)
		(size 2 3)
		(drill oval 1.1 1.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.25)
	)
	(pad "MP" thru_hole roundrect
		(at 5.8 7.25 180)
		(size 2 3)
		(drill oval 1.1 1.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.25)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Potentiometer_THT.3dshapes/Potentiometer_Alps_RK09L_Double_Horizontal.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
