(footprint "Potentiometer_Alps_RK163_Dual_Horizontal"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "12101A2 1210AX9 12A0B85 12A0BKR  Potentiometer, horizontal, Alps RK163 Dual, https://tech.alpsalpine.com/prod/e/pdf/potentiometer/rotarypotentiometers/rk16/rk16.pdf")
	(tags "Potentiometer horizontal Alps RK163 Dual")
	(property "Reference" "REF**"
		(at -0.000001 15.199999 180)
		(layer "F.SilkS")
	)
	(property "Value" "Potentiometer_Alps_RK163_Dual_Horizontal"
		(at 0 -5.2 180)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 2.25 5 180)
		(layer "F.Fab")
	)
	(pad "1" thru_hole rect
		(at 0 0 180)
		(size 3 3)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 0 5 180)
		(size 3 3)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at 0 10 180)
		(size 3 3)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 5 0 180)
		(size 3 3)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole circle
		(at 5 5 180)
		(size 3 3)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "6" thru_hole circle
		(at 5 10 180)
		(size 3 3)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Potentiometer_THT.3dshapes/Potentiometer_Alps_RK163_Dual_Horizontal.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
