(footprint "Potentiometer_Bourns_PTA4543_Single_Slide"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Bourns single-gang slide potentiometer, 45.0mm travel, https://www.bourns.com/docs/Product-Datasheets/pta.pdf")
	(tags "Bourns single-gang slide potentiometer 45.0mm")
	(property "Reference" "REF**"
		(at 29.25 -4 0)
		(layer "F.SilkS")
	)
	(property "Value" "Potentiometer_Bourns_PTA4543_Single_Slide"
		(at 29.25 7.5 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 29.25 1.75 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole rect
		(at 0 0)
		(size 1.75 1.75)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 0 3.5)
		(size 1.75 1.75)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at 58.5 0)
		(size 1.75 1.75)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "MP" thru_hole circle
		(at 4.15 5.95)
		(size 2.7 2.7)
		(drill 1.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "MP" thru_hole circle
		(at 5.35 -2.45)
		(size 2.7 2.7)
		(drill 1.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "MP" thru_hole circle
		(at 53.15 -2.45)
		(size 2.7 2.7)
		(drill 1.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "MP" thru_hole circle
		(at 54.35 5.95)
		(size 2.7 2.7)
		(drill 1.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Potentiometer_THT.3dshapes/Potentiometer_Bourns_PTA4543_Single_Slide.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
