(footprint "Potentiometer_Bourns_PTV09A-1_Single_Vertical"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Potentiometer, vertical, Bourns PTV09A-1 Single, http://www.bourns.com/docs/Product-Datasheets/ptv09.pdf")
	(tags "Potentiometer vertical Bourns PTV09A-1 Single")
	(property "Reference" "REF**"
		(at 6.05 -10.15 0)
		(layer "F.SilkS")
	)
	(property "Value" "Potentiometer_Bourns_PTV09A-1_Single_Vertical"
		(at 6.05 5.15 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 2 -2.5 90)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at 7 -6.9)
		(size 4 4)
		(drill 2.2)
		(layers "F&B.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 7 1.9)
		(size 4 4)
		(drill 2.2)
		(layers "F&B.Cu" "*.Mask")
	)
	(pad "1" thru_hole circle
		(at 0 0)
		(size 1.8 1.8)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 0 -2.5)
		(size 1.8 1.8)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at 0 -5)
		(size 1.8 1.8)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Potentiometer_THT.3dshapes/Potentiometer_Bourns_PTV09A-1_Single_Vertical.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
