(footprint "Potentiometer_Bourns_PTV09A-2_Single_Horizontal"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Potentiometer, horizontal, Bourns PTV09A-2 Single, http://www.bourns.com/docs/Product-Datasheets/ptv09.pdf")
	(tags "Potentiometer horizontal Bourns PTV09A-2 Single")
	(property "Reference" "REF**"
		(at 0 -11.05 0)
		(layer "F.SilkS")
	)
	(property "Value" "Potentiometer_Bourns_PTV09A-2_Single_Horizontal"
		(at 0 6.05 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 1 -2.5 0)
		(layer "F.Fab")
	)
	(pad "" thru_hole circle
		(at -3.3 -7.5)
		(size 4.6 4.6)
		(drill 2.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "" thru_hole circle
		(at -3.3 2.5)
		(size 4.6 4.6)
		(drill 2.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole circle
		(at 0 0)
		(size 1.8 1.8)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 0 -2.5)
		(size 1.8 1.8)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at 0 -5)
		(size 1.8 1.8)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Potentiometer_THT.3dshapes/Potentiometer_Bourns_PTV09A-2_Single_Horizontal.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
