(footprint "Potentiometer_Piher_PT-10-V10_Vertical_Hole"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Potentiometer, vertical, shaft hole, Piher PT-10-V10, http://www.piher-nacesa.com/pdf/12-PT10v03.pdf")
	(tags "Potentiometer vertical hole Piher PT-10-V10")
	(property "Reference" "REF**"
		(at 5 -9.05 0)
		(layer "F.SilkS")
	)
	(property "Value" "Potentiometer_Piher_PT-10-V10_Vertical_Hole"
		(at 5 3.75 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 1.05 -2.65 90)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at 5 -2.65)
		(size 4 4)
		(drill 4)
		(layers "*.Cu" "*.Mask")
	)
	(pad "1" thru_hole circle
		(at 0 0)
		(size 2.34 2.34)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 10 -2.5)
		(size 2.34 2.34)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at 0 -5)
		(size 2.34 2.34)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Potentiometer_THT.3dshapes/Potentiometer_Piher_PT-10-V10_Vertical_Hole.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
