(footprint "Abracon_APAES868R8060C16-T"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Abracon RHCP ceramic patch antenna 854-882Mhz, 5dBi")
	(tags "APAES patch antenna")
	(property "Reference" "${REFERENCE}"
		(at 0 11.5 0)
		(layer "F.Fab")
	)
	(property "Value" "Abracon_APAES868R8060C16-T"
		(at 0.127 13.159 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at -0.127 -31.037 0)
		(layer "F.SilkS")
	)
	(pad "1" thru_hole roundrect
		(at 0 0)
		(size 1.7 1.7)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.25)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/RF_Antenna.3dshapes/Abracon_APAES868R8060C16-T.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
