(footprint "Abracon_PRO-OB-471"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "OnBoard 868/915/868+2400 MHz Antenna, https://abracon.com/datasheets/PRO-OB-471.pdf")
	(tags "Antenna ProAnt OnBoard 868Mhz 915Mhz 2400Mhz")
	(property "Reference" "REF**"
		(at -15.115 7.04 180)
		(layer "F.SilkS")
	)
	(property "Value" "Abracon_PRO-OB-471"
		(at 0 -1.27 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 -2.56 0)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -11.5 -4.9)
		(size 1 1.95)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "2" smd roundrect
		(at -16.6 -4.9)
		(size 1 1.95)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "3" smd roundrect
		(at -11.5 4.9)
		(size 1 1.95)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "4" smd roundrect
		(at 12 4.9)
		(size 1 1.95)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "5" smd roundrect
		(at 12 -4.9)
		(size 1 1.95)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "6" smd roundrect
		(at -4.8 -4.9)
		(size 1 1.95)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F.Cu" "Dwgs.User")
		(hatch edge 0.508)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias not_allowed)
			(pads allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy -10.7 -3.65) (xy -12.3 -3.64) (xy -12.3 -6.15) (xy -10.7 -6.15)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F.Cu" "Dwgs.User")
		(hatch edge 0.508)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy -9.55 7.3) (xy -13.45 7.3) (xy -13.45 2.5) (xy -9.55 2.5)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F.Cu" "Dwgs.User")
		(hatch edge 0.508)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy -2.85 -2.5) (xy -6.75 -2.5) (xy -6.75 -7.3) (xy -2.85 -7.3)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F.Cu" "Dwgs.User")
		(hatch edge 0.508)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy 13.95 -2.5) (xy 10.05 -2.5) (xy 10.05 -7.3) (xy 13.95 -7.3)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F.Cu" "Dwgs.User")
		(hatch edge 0.508)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy 13.95 7.3) (xy 10.05 7.3) (xy 10.05 2.5) (xy 13.95 2.5)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F.Cu" "Dwgs.User")
		(hatch edge 0.508)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy -16.7 -5.875) (xy -17.1 -5.875) (xy -17.1 -5) (xy -17.4 -5) (xy -17.4 -6.15) (xy -16.7 -6.15)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F.Cu" "Dwgs.User")
		(hatch edge 0.508)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy -16.7 -3.925) (xy -17.1 -3.925) (xy -17.1 -4.8) (xy -17.4 -4.8) (xy -17.4 -3.65) (xy -16.7 -3.65)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F.Cu" "Dwgs.User")
		(hatch edge 0.508)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy -16.5 -5.875) (xy -16.1 -5.875) (xy -16.1 -5) (xy -15.8 -5) (xy -15.8 -6.15) (xy -16.5 -6.15)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F.Cu" "Dwgs.User")
		(hatch edge 0.508)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy -16.5 -3.925) (xy -16.1 -3.925) (xy -16.1 -4.8) (xy -15.8 -4.8) (xy -15.8 -3.65) (xy -16.5 -3.65)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "B.Cu" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu" "In7.Cu"
			"Dwgs.User" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu"
			"In14.Cu" "In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu"
			"In21.Cu" "In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu"
			"In28.Cu" "In29.Cu" "In30.Cu"
		)
		(hatch edge 0.508)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy -10.7 -3.65) (xy -12.3 -3.65) (xy -12.3 -6.15) (xy -10.7 -6.15)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "B.Cu" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu" "In7.Cu"
			"Dwgs.User" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu"
			"In14.Cu" "In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu"
			"In21.Cu" "In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu"
			"In28.Cu" "In29.Cu" "In30.Cu"
		)
		(hatch edge 0.508)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy -9.55 7.3) (xy -13.45 7.3) (xy -13.45 2.5) (xy -9.55 2.5)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "B.Cu" "In1.Cu" "Dwgs.User")
		(hatch edge 0.508)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy -2.85 -2.5) (xy -6.75 -2.5) (xy -6.75 -7.3) (xy -2.85 -7.3)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "B.Cu" "In1.Cu" "Dwgs.User")
		(hatch edge 0.508)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy 13.95 -2.5) (xy 10.05 -2.5) (xy 10.05 -7.3) (xy 13.95 -7.3)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "B.Cu" "In1.Cu" "Dwgs.User")
		(hatch edge 0.508)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy 13.95 7.3) (xy 10.05 7.3) (xy 10.05 2.5) (xy 13.95 2.5)
			)
		)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/RF_Antenna.3dshapes/Abracon_PRO-OB-471.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
