(footprint "Antenova_SR4G013_GPS"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "GPS/GLONASS/Galileo/BeiDou antenna, 1559-1609Mhz, SMD, https://www.application-datasheet.com/pdf/antenova/sr4g013.pdf")
	(tags "antenna GPS Antenova Beltii")
	(property "Reference" "REF**"
		(at 0 2.8 180)
		(layer "F.SilkS")
	)
	(property "Value" "Antenova_SR4G013_GPS"
		(at 0 3.04 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(net_tie_pad_groups "1, 2")
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -6.9 0)
		(size 1.2 3.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2083333333)
	)
	(pad "2" smd roundrect
		(at -8.05 0)
		(size 0.3 0.3)
		(layers "F.Cu")
		(roundrect_rratio 0.25)
		(zone_connect 2)
		(thermal_bridge_angle 45)
	)
	(pad "2" smd roundrect
		(at -2.3 0)
		(size 1.2 3.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2083333333)
		(thermal_bridge_width 0.5)
	)
	(pad "2" smd roundrect
		(at 2.3 0)
		(size 1.2 3.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2083333333)
		(thermal_bridge_width 0.5)
	)
	(pad "2" smd roundrect
		(at 6.9 0)
		(size 1.2 3.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2083333333)
		(thermal_bridge_width 0.5)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(hatch edge 0.508)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy -7.45 -1.65) (xy -6.25 -1.65) (xy -6.25 1.6) (xy -6.15 1.6) (xy -6.15 -1.75) (xy -7.45 -1.75)
			)
		)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/RF_Antenna.3dshapes/Antenova_SR4G013_GPS.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
