(footprint "Astrocast_AST50127-00"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "L-band patch antenna, https://docs.astrocast.com/dl/0534-DOC-M2M-ASTRO-Patch_Antenna-Datasheet.pdf")
	(tags "L-band antenna astrocast Patch Antenna")
	(property "Reference" "REF**"
		(at -14.84 -14.03 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(property "Value" "Astrocast_AST50127-00"
		(at 0 14.86 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "Antenna keepout"
		(at -6.31 5.26 0)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "${REFERENCE}"
		(at 0 4.7 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole circle
		(at 0 0)
		(size 1.6 1.6)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(name "Antenna Keepout")
		(hatch full 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias allowed)
			(pads not_allowed)
			(copperpour allowed)
			(footprints not_allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy -17.5 -12.8) (xy -17.5 22.2) (xy 17.5 22.2) (xy 17.5 -12.8)
			)
		)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/RF_Antenna.3dshapes/Astrocast_AST50127-00.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
