(footprint "Johanson_2450AT18x100"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Johanson 2450AT43F0100 SMD antenna 2400-2500Mhz, -0.5dBi, https://www.johansontechnology.com/datasheets/2450AT18A100/2450AT18A100.pdf")
	(tags "antenna")
	(property "Reference" "REF**"
		(at 0 -1.85 0)
		(layer "F.SilkS")
	)
	(property "Value" "Johanson_2450AT18x100"
		(at 0 1.85 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -1.45 0)
		(size 1.2 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.208333)
	)
	(pad "2" smd roundrect
		(at 1.45 0)
		(size 1.2 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.208333)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/RF_Antenna.3dshapes/Johanson_2450AT18x100.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
