(footprint "NiceRF_SW868-TH13_868Mhz"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "868Mhz copper string antenna, right angle, approx. 15mm coil length, 5.5mm OD, 0.8 wire diameter, https://www.nicerf.com/item/868mhz-spring-antenna-sw868-th13")
	(tags "antenna rf")
	(property "Reference" "REF**"
		(at 0 2 0)
		(layer "F.SilkS")
	)
	(property "Value" "NiceRF_SW868-TH13_868Mhz"
		(at 12.75 3.7 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 12.75 0 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole roundrect
		(at 0 0 270)
		(size 1.5 1.5)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.1640419948)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/RF_Antenna.3dshapes/NiceRF_SW868-TH13_868Mhz.wrl"
		(hide yes)
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
