(footprint "Texas_SWRA416_868MHz_915MHz"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "http://www.ti.com/lit/an/swra416/swra416.pdf")
	(tags "PCB antenna")
	(property "Reference" "REF**"
		(at -6 6.6 0)
		(layer "F.SilkS")
	)
	(property "Value" "Texas_SWRA416_868MHz_915MHz"
		(at 0.1 -7.6 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user " any PCB layer."
		(at 1 4.2 0)
		(layer "Cmts.User")
	)
	(fp_text user "KEEP-OUT ZONE"
		(at 1 -2.8 0)
		(layer "Cmts.User")
	)
	(fp_text user "No metal, traces or "
		(at 1 0.2 0)
		(layer "Cmts.User")
	)
	(fp_text user "any components on"
		(at 1 2.2 0)
		(layer "Cmts.User")
	)
	(fp_text user "${REFERENCE}"
		(at -0.4 6.6 0)
		(layer "F.Fab")
	)
	(pad "" thru_hole circle
		(at -9 -5.8 180)
		(size 1 1)
		(drill 0.4)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "" thru_hole circle
		(at -7 -5.8 180)
		(size 1 1)
		(drill 0.4)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "" thru_hole circle
		(at -7 -0.8 180)
		(size 1 1)
		(drill 0.4)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "" thru_hole circle
		(at -5 -5.8 180)
		(size 1 1)
		(drill 0.4)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "" thru_hole circle
		(at -5 -0.8 180)
		(size 1 1)
		(drill 0.4)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "" thru_hole circle
		(at -3 -5.8 180)
		(size 1 1)
		(drill 0.4)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "" thru_hole circle
		(at -3 -0.8 180)
		(size 1 1)
		(drill 0.4)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "" thru_hole circle
		(at -1 -5.8 180)
		(size 1 1)
		(drill 0.4)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "" thru_hole circle
		(at -1 -0.8 180)
		(size 1 1)
		(drill 0.4)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "" thru_hole circle
		(at 1 -5.8 180)
		(size 1 1)
		(drill 0.4)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "" thru_hole circle
		(at 1 -0.8 180)
		(size 1 1)
		(drill 0.4)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "" thru_hole circle
		(at 3 -5.8 180)
		(size 1 1)
		(drill 0.4)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "" thru_hole circle
		(at 3 -0.8 180)
		(size 1 1)
		(drill 0.4)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "" thru_hole circle
		(at 5 -5.8 180)
		(size 1 1)
		(drill 0.4)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "" thru_hole circle
		(at 5 -0.8 180)
		(size 1 1)
		(drill 0.4)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "" thru_hole circle
		(at 7 -5.8 180)
		(size 1 1)
		(drill 0.4)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "" thru_hole circle
		(at 7 -0.8 180)
		(size 1 1)
		(drill 0.4)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "" thru_hole circle
		(at 9 -5.8 180)
		(size 1 1)
		(drill 0.4)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "" thru_hole circle
		(at 9 -0.8 180)
		(size 1 1)
		(drill 0.4)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "1" smd trapezoid
		(at -9 5.9 180)
		(size 0.4 0.8)
		(rect_delta 0 0.3)
		(layers "F.Cu")
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(hatch full 0.508)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour not_allowed)
			(footprints not_allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy -9.7 5.7) (xy 9.7 5.7) (xy 9.7 -6.5) (xy -9.7 -6.5)
			)
		)
	)
	(embedded_fonts no)
)
