(footprint "Balun_Johanson_0896BM15A0001"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "https://www.johansontechnology.com/datasheets/0896BM15A0001/0896BM15A0001.pdf")
	(tags "balun RF")
	(property "Reference" "REF**"
		(at 0 -2 0)
		(layer "F.SilkS")
	)
	(property "Value" "Balun_Johanson_0896BM15A0001"
		(at 0 2 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0.05 -0.1 90)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -0.9 -0.65)
		(size 1 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(clearance 0.2)
	)
	(pad "2" smd rect
		(at -0.9 0)
		(size 1 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -0.9 0.65)
		(size 1 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(clearance 0.2)
	)
	(pad "4" smd rect
		(at 0.9 0.65)
		(size 1 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(clearance 0.2)
	)
	(pad "5" smd rect
		(at 0.9 0)
		(size 1 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at 0.9 -0.65)
		(size 1 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(clearance 0.2)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/RF_Converter.3dshapes/Balun_Johanson_0896BM15A0001.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
