(footprint "Balun_Johanson_0900PC15J0013"
	(version 20240108)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "Johanson 0900PC15J0013 DFN, 10 Pin (https://www.johansontechnology.com/datasheets/0900PC15J0013/0900PC15J0013.pdf), generated with kicad-footprint-generator ipc_noLead_generator.py")
	(tags "Johanson DFN NoLead")
	(property "Reference" "REF**"
		(at 0 -2.35 0)
		(layer "F.SilkS")
	)
	(property "Value" "Balun_Johanson_0900PC15J0013"
		(at 0 2.35 0)
		(layer "F.Fab")
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 90)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -0.7125 -0.75)
		(size 0.625 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "2" smd roundrect
		(at -0.7125 -0.25)
		(size 0.625 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "3" smd roundrect
		(at -0.7125 0.25)
		(size 0.625 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "4" smd roundrect
		(at -0.7125 0.75)
		(size 0.625 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "5" smd roundrect
		(at 0 1.0875)
		(size 0.3 0.625)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "6" smd roundrect
		(at 0.7125 0.75)
		(size 0.625 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "7" smd roundrect
		(at 0.7125 0.25)
		(size 0.625 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "8" smd roundrect
		(at 0.7125 -0.25)
		(size 0.625 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "9" smd roundrect
		(at 0.7125 -0.75)
		(size 0.625 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "10" smd roundrect
		(at 0 -1.0875)
		(size 0.3 0.625)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(model "${KICAD9_3DMODEL_DIR}/RF_Converter.3dshapes/Balun_Johanson_0900PC15J0013.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
