(footprint "OriginGPS_ORG1510"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "GPS / GNSS Module with integrated antenna, (https://origingps.com/wp-content/uploads/2019/09/HORNET-Modules-Layout-recommendations-and-Integration-Application-Note-Rev-2.0.pdf)")
	(tags "GPS GNSS OriginGPS Hornet")
	(property "Reference" "REF**"
		(at 0 -6 0)
		(layer "F.SilkS")
	)
	(property "Value" "OriginGPS_ORG1510"
		(at 0 6 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -4.362 -2.54)
		(size 1.676 0.864)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "2" smd roundrect
		(at -4.489 -1.27)
		(size 1.422 0.864)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "3" smd roundrect
		(at -4.489 0)
		(size 1.422 0.864)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "4" smd roundrect
		(at -4.489 1.27)
		(size 1.422 0.864)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "5" smd roundrect
		(at -4.489 2.54)
		(size 1.422 0.864)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "6" smd roundrect
		(at 4.489 2.54)
		(size 1.422 0.864)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "7" smd roundrect
		(at 4.489 1.27)
		(size 1.422 0.864)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "8" smd roundrect
		(at 4.489 0)
		(size 1.422 0.864)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "9" smd roundrect
		(at 4.489 -1.27)
		(size 1.422 0.864)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "10" smd roundrect
		(at 4.489 -2.54)
		(size 1.422 0.864)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "11" thru_hole circle
		(at -2.5 -3.75)
		(size 1.2 1.2)
		(drill 0.5)
		(layers "*.Cu" "B.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole circle
		(at -2.5 -1.25 90)
		(size 1.2 1.2)
		(drill 0.5)
		(layers "*.Cu" "B.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole circle
		(at -2.5 1.25 90)
		(size 1.2 1.2)
		(drill 0.5)
		(layers "*.Cu" "B.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole circle
		(at -2.5 3.75 90)
		(size 1.2 1.2)
		(drill 0.5)
		(layers "*.Cu" "B.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole circle
		(at 0 -3.75)
		(size 1.2 1.2)
		(drill 0.5)
		(layers "*.Cu" "B.Mask")
		(remove_unused_layers no)
	)
	(pad "11" smd custom
		(at 0 -2.665)
		(size 0.6 0.6)
		(layers "F.Cu")
		(zone_connect 0)
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0.889 3.363) (xy 0.871 3.177) (xy 0.815 2.999) (xy 0.722 2.836) (xy 0.598 2.697) (xy 0.447 2.586)
					(xy 0.276 2.51) (xy 0.093 2.471) (xy -0.093 2.471) (xy -0.276 2.51) (xy -0.447 2.586) (xy -0.598 2.697)
					(xy -0.722 2.836) (xy -0.815 2.999) (xy -0.871 3.177) (xy -0.889 3.363) (xy -3.175 3.363) (xy -3.175 -1.78)
					(xy 3.175 -1.78) (xy 3.175 3.363)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "11" thru_hole circle
		(at 0 -1.25)
		(size 1.2 1.2)
		(drill 0.5)
		(layers "*.Cu" "B.Mask")
		(remove_unused_layers no)
	)
	(pad "11" smd custom
		(at 0 3.442 90)
		(size 0.5 0.5)
		(layers "F.Cu")
		(zone_connect 0)
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy 2.571 -0.87) (xy 2.406 -0.819) (xy 2.254 -0.736) (xy 2.12 -0.626) (xy 2.011 -0.491) (xy 1.93 -0.338)
					(xy 1.88 -0.172) (xy 1.863 0) (xy 1.88 0.172) (xy 1.93 0.338) (xy 2.011 0.491) (xy 2.12 0.626)
					(xy 2.254 0.736) (xy 2.406 0.819) (xy 2.571 0.87) (xy 2.744 0.889) (xy 2.744 3.175) (xy -1.003 3.175)
					(xy -1.003 -3.175) (xy 2.744 -3.175) (xy 2.744 -0.889)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "11" thru_hole circle
		(at 0 3.75)
		(size 1.2 1.2)
		(drill 0.5)
		(layers "*.Cu" "B.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole circle
		(at 2.5 -3.75)
		(size 1.2 1.2)
		(drill 0.5)
		(layers "*.Cu" "B.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole circle
		(at 2.5 -1.25)
		(size 1.2 1.2)
		(drill 0.5)
		(layers "*.Cu" "B.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole circle
		(at 2.5 1.25)
		(size 1.2 1.2)
		(drill 0.5)
		(layers "*.Cu" "B.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole circle
		(at 2.5 3.75 90)
		(size 1.2 1.2)
		(drill 0.5)
		(layers "*.Cu" "B.Mask")
		(remove_unused_layers no)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy -0.889 0.698) (xy -0.871 0.512) (xy -0.815 0.334) (xy -0.722 0.171) (xy -0.598 0.032) (xy -0.447 -0.079)
				(xy -0.276 -0.155) (xy -0.093 -0.194) (xy 0.093 -0.194) (xy 0.276 -0.155) (xy 0.447 -0.079) (xy 0.598 0.032)
				(xy 0.722 0.171) (xy 0.815 0.334) (xy 0.871 0.512) (xy 0.889 0.698) (xy 0.87 0.871) (xy 0.819 1.036)
				(xy 0.736 1.188) (xy 0.626 1.322) (xy 0.491 1.431) (xy 0.338 1.512) (xy 0.172 1.562) (xy 0 1.579)
				(xy -0.172 1.562) (xy -0.338 1.512) (xy -0.491 1.431) (xy -0.626 1.322) (xy -0.736 1.188) (xy -0.819 1.036)
				(xy -0.87 0.871)
			)
		)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/RF_GPS.3dshapes/OriginGPS_ORG1510.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
