(footprint "Quectel_L80-R"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Quectel L80-R GPS Module, Patch on Top, https://www.quectel.com/UploadImage/Downlad/Quectel_L80-R_Hardware_Design_V1.2.pdf")
	(tags "quectel GPS GNSS")
	(property "Reference" "REF**"
		(at 0 -9 180)
		(layer "F.SilkS")
	)
	(property "Value" "Quectel_L80-R"
		(at 0 9 180)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "Keepout"
		(at -0.6 -0.63 0)
		(layer "Cmts.User")
	)
	(fp_text user "${REFERENCE}"
		(at 0 2.032 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -7.75 -5.85 180)
		(size 2.5 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -7.75 -3.31 180)
		(size 2.5 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -7.75 -0.77 180)
		(size 2.5 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -7.75 1.77 180)
		(size 2.5 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at -7.75 4.31 180)
		(size 2.5 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at -7.75 6.85 180)
		(size 2.5 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at 7.75 6.85 180)
		(size 2.5 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at 7.75 4.31 180)
		(size 2.5 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at 7.75 1.77 180)
		(size 2.5 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd rect
		(at 7.75 -0.77 180)
		(size 2.5 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd rect
		(at 7.75 -3.31 180)
		(size 2.5 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "12" smd rect
		(at 7.75 -5.85 180)
		(size 2.5 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(hatch full 0.508)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints not_allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy 0.654775 -0.63) (xy 0.635712 -0.847889) (xy 0.579103 -1.059158) (xy 0.486667 -1.257387) (xy 0.361213 -1.436554)
				(xy 0.206554 -1.591213) (xy 0.027388 -1.716667) (xy -0.170842 -1.809103) (xy -0.382111 -1.865712)
				(xy -0.6 -1.884775) (xy -0.817889 -1.865712) (xy -1.029158 -1.809103) (xy -1.227387 -1.716667) (xy -1.406554 -1.591213)
				(xy -1.561213 -1.436554) (xy -1.686667 -1.257387) (xy -1.779103 -1.059158) (xy -1.835712 -0.847889)
				(xy -1.854775 -0.63) (xy -1.835712 -0.412111) (xy -1.779103 -0.200842) (xy -1.686667 -0.002613)
				(xy -1.561213 0.176554) (xy -1.406554 0.331213) (xy -1.227388 0.456667) (xy -1.029158 0.549103)
				(xy -0.817889 0.605712) (xy -0.6 0.624775) (xy -0.382111 0.605712) (xy -0.170842 0.549103) (xy 0.027388 0.456667)
				(xy 0.206554 0.331213) (xy 0.361213 0.176554) (xy 0.486667 -0.002613) (xy 0.579103 -0.200842) (xy 0.635712 -0.412111)
			)
		)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/RF_GPS.3dshapes/Quectel_L80-R.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
