(footprint "ublox_SAM-M8Q"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "GPS Module, 15.5x15.5x6.3mm, https://www.u-blox.com/sites/default/files/SAM-M8Q_HardwareIntegrationManual_%28UBX-16018358%29.pdf")
	(tags "ublox SAM-M8Q")
	(property "Reference" "REF**"
		(at 0 -8.75 0)
		(layer "F.SilkS")
	)
	(property "Value" "ublox_SAM-M8Q"
		(at 0 8.75 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(solder_mask_margin 0.000001)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" smd rect
		(at -7.1 -4.225)
		(size 0.72 0.58)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -7.1 -3.375)
		(size 0.72 0.58)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -7.1 -2.325)
		(size 0.72 0.58)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -7.1 -1.475)
		(size 0.72 0.58)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -7.1 -0.425)
		(size 0.72 0.58)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -7.1 0.425)
		(size 0.72 0.58)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -7.1 1.475)
		(size 0.72 0.58)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -7.1 2.325)
		(size 0.72 0.58)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -7.1 3.375)
		(size 0.72 0.58)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -7.1 4.225)
		(size 0.72 0.58)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -6.1 -4.225)
		(size 0.72 0.58)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -6.1 -3.375)
		(size 0.72 0.58)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -6.1 -2.325)
		(size 0.72 0.58)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -6.1 -1.475)
		(size 0.72 0.58)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -6.1 -0.425)
		(size 0.72 0.58)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -6.1 0.425)
		(size 0.72 0.58)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -6.1 1.475)
		(size 0.72 0.58)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -6.1 2.325)
		(size 0.72 0.58)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -6.1 3.375)
		(size 0.72 0.58)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -6.1 4.225)
		(size 0.72 0.58)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -4.225 -7.1)
		(size 0.58 0.72)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -4.225 -6.1)
		(size 0.58 0.72)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -4.225 6.1)
		(size 0.58 0.72)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -4.225 7.1)
		(size 0.58 0.72)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -3.375 -7.1)
		(size 0.58 0.72)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -3.375 -6.1)
		(size 0.58 0.72)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -3.375 6.1)
		(size 0.58 0.72)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -3.375 7.1)
		(size 0.58 0.72)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -2.325 -7.1)
		(size 0.58 0.72)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -2.325 -6.1)
		(size 0.58 0.72)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -2.325 6.1)
		(size 0.58 0.72)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -2.325 7.1)
		(size 0.58 0.72)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -1.475 -7.1)
		(size 0.58 0.72)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -1.475 -6.1)
		(size 0.58 0.72)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -1.475 6.1)
		(size 0.58 0.72)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -1.475 7.1)
		(size 0.58 0.72)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -0.425 -7.1)
		(size 0.58 0.72)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -0.425 -6.1)
		(size 0.58 0.72)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -0.425 6.1)
		(size 0.58 0.72)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -0.425 7.1)
		(size 0.58 0.72)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0.425 -7.1)
		(size 0.58 0.72)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0.425 -6.1)
		(size 0.58 0.72)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0.425 6.1)
		(size 0.58 0.72)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0.425 7.1)
		(size 0.58 0.72)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 1.475 -7.1)
		(size 0.58 0.72)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 1.475 -6.1)
		(size 0.58 0.72)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 1.475 6.1)
		(size 0.58 0.72)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 1.475 7.1)
		(size 0.58 0.72)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 2.325 -7.1)
		(size 0.58 0.72)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 2.325 -6.1)
		(size 0.58 0.72)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 2.325 6.1)
		(size 0.58 0.72)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 2.325 7.1)
		(size 0.58 0.72)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 3.375 -7.1)
		(size 0.58 0.72)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 3.375 -6.1)
		(size 0.58 0.72)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 3.375 6.1)
		(size 0.58 0.72)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 3.375 7.1)
		(size 0.58 0.72)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 4.225 -7.1)
		(size 0.58 0.72)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 4.225 -6.1)
		(size 0.58 0.72)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 4.225 6.1)
		(size 0.58 0.72)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 4.225 7.1)
		(size 0.58 0.72)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 6.1 -4.225)
		(size 0.72 0.58)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 6.1 -3.375)
		(size 0.72 0.58)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 6.1 -2.325)
		(size 0.72 0.58)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 6.1 -1.475)
		(size 0.72 0.58)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 6.1 -0.425)
		(size 0.72 0.58)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 6.1 0.425)
		(size 0.72 0.58)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 6.1 1.475)
		(size 0.72 0.58)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 6.1 2.325)
		(size 0.72 0.58)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 6.1 3.375)
		(size 0.72 0.58)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 6.1 4.225)
		(size 0.72 0.58)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 7.1 -4.225)
		(size 0.72 0.58)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 7.1 -3.375)
		(size 0.72 0.58)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 7.1 -2.325)
		(size 0.72 0.58)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 7.1 -1.475)
		(size 0.72 0.58)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 7.1 -0.425)
		(size 0.72 0.58)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 7.1 0.425)
		(size 0.72 0.58)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 7.1 1.475)
		(size 0.72 0.58)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 7.1 2.325)
		(size 0.72 0.58)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 7.1 3.375)
		(size 0.72 0.58)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 7.1 4.225)
		(size 0.72 0.58)
		(layers "F.Paste")
	)
	(pad "1" smd rect
		(at -6.6 -3.8)
		(size 1.8 1.5)
		(layers "F.Cu" "F.Mask")
	)
	(pad "2" smd rect
		(at -6.6 -1.9)
		(size 1.8 1.5)
		(layers "F.Cu" "F.Mask")
	)
	(pad "3" smd rect
		(at -6.6 0)
		(size 1.8 1.5)
		(layers "F.Cu" "F.Mask")
	)
	(pad "4" smd rect
		(at -6.6 1.9)
		(size 1.8 1.5)
		(layers "F.Cu" "F.Mask")
	)
	(pad "5" smd rect
		(at -6.6 3.8)
		(size 1.8 1.5)
		(layers "F.Cu" "F.Mask")
	)
	(pad "6" smd rect
		(at -3.8 6.6)
		(size 1.5 1.8)
		(layers "F.Cu" "F.Mask")
	)
	(pad "7" smd rect
		(at -1.9 6.6)
		(size 1.5 1.8)
		(layers "F.Cu" "F.Mask")
	)
	(pad "8" smd rect
		(at 0 6.6)
		(size 1.5 1.8)
		(layers "F.Cu" "F.Mask")
	)
	(pad "9" smd rect
		(at 1.9 6.6)
		(size 1.5 1.8)
		(layers "F.Cu" "F.Mask")
	)
	(pad "10" smd rect
		(at 3.8 6.6)
		(size 1.5 1.8)
		(layers "F.Cu" "F.Mask")
	)
	(pad "11" smd rect
		(at 6.6 3.8)
		(size 1.8 1.5)
		(layers "F.Cu" "F.Mask")
	)
	(pad "12" smd rect
		(at 6.6 1.9)
		(size 1.8 1.5)
		(layers "F.Cu" "F.Mask")
	)
	(pad "13" smd rect
		(at 6.6 0)
		(size 1.8 1.5)
		(layers "F.Cu" "F.Mask")
	)
	(pad "14" smd rect
		(at 6.6 -1.9)
		(size 1.8 1.5)
		(layers "F.Cu" "F.Mask")
	)
	(pad "15" smd rect
		(at 6.6 -3.8)
		(size 1.8 1.5)
		(layers "F.Cu" "F.Mask")
	)
	(pad "16" smd rect
		(at 3.8 -6.6)
		(size 1.5 1.8)
		(layers "F.Cu" "F.Mask")
	)
	(pad "17" smd rect
		(at 1.9 -6.6)
		(size 1.5 1.8)
		(layers "F.Cu" "F.Mask")
	)
	(pad "18" smd rect
		(at 0 -6.6)
		(size 1.5 1.8)
		(layers "F.Cu" "F.Mask")
	)
	(pad "19" smd rect
		(at -1.9 -6.6)
		(size 1.5 1.8)
		(layers "F.Cu" "F.Mask")
	)
	(pad "20" smd rect
		(at -3.8 -6.6)
		(size 1.5 1.8)
		(layers "F.Cu" "F.Mask")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/RF_GPS.3dshapes/ublox_SAM-M8Q.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
