(footprint "Quectel_BC66"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "GSM NB-IoT module, 15.8x17.7x2mm, https://www.quectel.com/UploadImage/Downlad/Quectel_BC66_Hardware_Design_V1.1.pdf")
	(tags "GSM NB-IoT Module BC66 M66")
	(property "Reference" "REF**"
		(at 0 -12.6 0)
		(layer "F.SilkS")
	)
	(property "Value" "Quectel_BC66"
		(at 0 12.6 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" smd roundrect
		(at -8.05 -6.6)
		(size 2.9 0.595)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at -8.05 -5.5)
		(size 2.9 0.595)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at -8.05 -4.4)
		(size 2.9 0.595)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at -8.05 -3.3)
		(size 2.9 0.595)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at -8.05 -2.2)
		(size 2.9 0.595)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at -8.05 -1.1)
		(size 2.9 0.595)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at -8.05 0)
		(size 2.9 0.595)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at -8.05 1.1)
		(size 2.9 0.595)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at -8.05 2.2)
		(size 2.9 0.595)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at -8.05 3.3)
		(size 2.9 0.595)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at -8.05 4.4)
		(size 2.9 0.595)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at -8.05 5.5)
		(size 2.9 0.595)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at -8.05 6.6)
		(size 2.9 0.595)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at -4.4 -9 90)
		(size 2.9 0.595)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at -4.4 9 90)
		(size 2.9 0.595)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd circle
		(at -3.6 -2.7)
		(size 0.9 0.9)
		(layers "F.Paste")
	)
	(pad "" smd circle
		(at -3.6 -0.9)
		(size 0.9 0.9)
		(layers "F.Paste")
	)
	(pad "" smd circle
		(at -3.6 0.9)
		(size 0.9 0.9)
		(layers "F.Paste")
	)
	(pad "" smd circle
		(at -3.6 2.7)
		(size 0.9 0.9)
		(layers "F.Paste")
	)
	(pad "" smd roundrect
		(at -3.3 -9 90)
		(size 2.9 0.595)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at -3.3 9 90)
		(size 2.9 0.595)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at -2.2 -9 90)
		(size 2.9 0.595)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at -2.2 9 90)
		(size 2.9 0.595)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd circle
		(at -1.8 -4.5)
		(size 0.9 0.9)
		(layers "F.Paste")
	)
	(pad "" smd circle
		(at -1.8 4.5)
		(size 0.9 0.9)
		(layers "F.Paste")
	)
	(pad "" smd roundrect
		(at -1.1 -9 90)
		(size 2.9 0.595)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at -1.1 9 90)
		(size 2.9 0.595)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 0 -9 90)
		(size 2.9 0.595)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd circle
		(at 0 -4.5)
		(size 0.9 0.9)
		(layers "F.Paste")
	)
	(pad "" smd circle
		(at 0 4.5)
		(size 0.9 0.9)
		(layers "F.Paste")
	)
	(pad "" smd roundrect
		(at 0 9 90)
		(size 2.9 0.595)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 1.1 -9 90)
		(size 2.9 0.595)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 1.1 9 90)
		(size 2.9 0.595)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd circle
		(at 1.8 -4.5)
		(size 0.9 0.9)
		(layers "F.Paste")
	)
	(pad "" smd circle
		(at 1.8 4.5)
		(size 0.9 0.9)
		(layers "F.Paste")
	)
	(pad "" smd roundrect
		(at 2.2 -9 90)
		(size 2.9 0.595)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 2.2 9 90)
		(size 2.9 0.595)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 3.3 -9 90)
		(size 2.9 0.595)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 3.3 9 90)
		(size 2.9 0.595)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd circle
		(at 3.6 -2.7)
		(size 0.9 0.9)
		(layers "F.Paste")
	)
	(pad "" smd circle
		(at 3.6 -0.9)
		(size 0.9 0.9)
		(layers "F.Paste")
	)
	(pad "" smd circle
		(at 3.6 0.9)
		(size 0.9 0.9)
		(layers "F.Paste")
	)
	(pad "" smd circle
		(at 3.6 2.7)
		(size 0.9 0.9)
		(layers "F.Paste")
	)
	(pad "" smd roundrect
		(at 4.4 -9 90)
		(size 2.9 0.595)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 4.4 9 90)
		(size 2.9 0.595)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 8.05 -6.6)
		(size 2.9 0.595)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 8.05 -5.5)
		(size 2.9 0.595)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 8.05 -4.4)
		(size 2.9 0.595)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 8.05 -3.3)
		(size 2.9 0.595)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 8.05 -2.2)
		(size 2.9 0.595)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 8.05 -1.1)
		(size 2.9 0.595)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 8.05 0)
		(size 2.9 0.595)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 8.05 1.1)
		(size 2.9 0.595)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 8.05 2.2)
		(size 2.9 0.595)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 8.05 3.3)
		(size 2.9 0.595)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 8.05 4.4)
		(size 2.9 0.595)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 8.05 5.5)
		(size 2.9 0.595)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 8.05 6.6)
		(size 2.9 0.595)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "1" smd roundrect
		(at -7.65 -6.6)
		(size 2.5 0.7)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "2" smd roundrect
		(at -7.65 -5.5)
		(size 2.5 0.7)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "3" smd roundrect
		(at -7.65 -4.4)
		(size 2.5 0.7)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "4" smd roundrect
		(at -7.65 -3.3)
		(size 2.5 0.7)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "5" smd roundrect
		(at -7.65 -2.2)
		(size 2.5 0.7)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "6" smd roundrect
		(at -7.65 -1.1)
		(size 2.5 0.7)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "7" smd roundrect
		(at -7.65 0)
		(size 2.5 0.7)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "8" smd roundrect
		(at -7.65 1.1)
		(size 2.5 0.7)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "9" smd roundrect
		(at -7.65 2.2)
		(size 2.5 0.7)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "10" smd roundrect
		(at -7.65 3.3)
		(size 2.5 0.7)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "11" smd roundrect
		(at -7.65 4.4)
		(size 2.5 0.7)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "12" smd roundrect
		(at -7.65 5.5)
		(size 2.5 0.7)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "13" smd roundrect
		(at -7.65 6.6)
		(size 2.5 0.7)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "14" smd roundrect
		(at -4.4 8.6 90)
		(size 2.5 0.7)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "15" smd roundrect
		(at -3.3 8.6 90)
		(size 2.5 0.7)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "16" smd roundrect
		(at -2.2 8.6 90)
		(size 2.5 0.7)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "17" smd roundrect
		(at -1.1 8.6 90)
		(size 2.5 0.7)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "18" smd roundrect
		(at 0 8.6 90)
		(size 2.5 0.7)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "19" smd roundrect
		(at 1.1 8.6 90)
		(size 2.5 0.7)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "20" smd roundrect
		(at 2.2 8.6 90)
		(size 2.5 0.7)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "21" smd roundrect
		(at 3.3 8.6 90)
		(size 2.5 0.7)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "22" smd roundrect
		(at 4.4 8.6 90)
		(size 2.5 0.7)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "23" smd roundrect
		(at 7.65 6.6)
		(size 2.5 0.7)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "24" smd roundrect
		(at 7.65 5.5)
		(size 2.5 0.7)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "25" smd roundrect
		(at 7.65 4.4)
		(size 2.5 0.7)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "26" smd roundrect
		(at 7.65 3.3)
		(size 2.5 0.7)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "27" smd roundrect
		(at 7.65 2.2)
		(size 2.5 0.7)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "28" smd roundrect
		(at 7.65 1.1)
		(size 2.5 0.7)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "29" smd roundrect
		(at 7.65 0)
		(size 2.5 0.7)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "30" smd roundrect
		(at 7.65 -1.1)
		(size 2.5 0.7)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "31" smd roundrect
		(at 7.65 -2.2)
		(size 2.5 0.7)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "32" smd roundrect
		(at 7.65 -3.3)
		(size 2.5 0.7)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "33" smd roundrect
		(at 7.65 -4.4)
		(size 2.5 0.7)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "34" smd roundrect
		(at 7.65 -5.5)
		(size 2.5 0.7)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "35" smd roundrect
		(at 7.65 -6.6)
		(size 2.5 0.7)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "36" smd roundrect
		(at 4.4 -8.6 270)
		(size 2.5 0.7)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "37" smd roundrect
		(at 3.3 -8.6 270)
		(size 2.5 0.7)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "38" smd roundrect
		(at 2.2 -8.6 270)
		(size 2.5 0.7)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "39" smd roundrect
		(at 1.1 -8.6 270)
		(size 2.5 0.7)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "40" smd roundrect
		(at 0 -8.6 270)
		(size 2.5 0.7)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "41" smd roundrect
		(at -1.1 -8.6 270)
		(size 2.5 0.7)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "42" smd roundrect
		(at -2.2 -8.6 270)
		(size 2.5 0.7)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "43" smd roundrect
		(at -3.3 -8.6 270)
		(size 2.5 0.7)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "44" smd roundrect
		(at -4.4 -8.6 270)
		(size 2.5 0.7)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "45" smd rect
		(at -3.6 -2.7)
		(size 1 1)
		(layers "F.Cu" "F.Mask")
	)
	(pad "46" smd rect
		(at -3.6 -0.9)
		(size 1 1)
		(layers "F.Cu" "F.Mask")
	)
	(pad "47" smd rect
		(at -3.6 0.9)
		(size 1 1)
		(layers "F.Cu" "F.Mask")
	)
	(pad "48" smd rect
		(at -3.6 2.7)
		(size 1 1)
		(layers "F.Cu" "F.Mask")
	)
	(pad "49" smd rect
		(at -1.8 4.5)
		(size 1 1)
		(layers "F.Cu" "F.Mask")
	)
	(pad "50" smd rect
		(at 0 4.5)
		(size 1 1)
		(layers "F.Cu" "F.Mask")
	)
	(pad "51" smd rect
		(at 1.8 4.5)
		(size 1 1)
		(layers "F.Cu" "F.Mask")
	)
	(pad "52" smd rect
		(at 3.6 2.7)
		(size 1 1)
		(layers "F.Cu" "F.Mask")
	)
	(pad "53" smd rect
		(at 3.6 0.9)
		(size 1 1)
		(layers "F.Cu" "F.Mask")
	)
	(pad "54" smd rect
		(at 3.6 -0.9)
		(size 1 1)
		(layers "F.Cu" "F.Mask")
	)
	(pad "55" smd rect
		(at 3.6 -2.7)
		(size 1 1)
		(layers "F.Cu" "F.Mask")
	)
	(pad "56" smd rect
		(at 1.8 -4.5)
		(size 1 1)
		(layers "F.Cu" "F.Mask")
	)
	(pad "57" smd rect
		(at 0 -4.5)
		(size 1 1)
		(layers "F.Cu" "F.Mask")
	)
	(pad "58" smd rect
		(at -1.8 -4.5)
		(size 1 1)
		(layers "F.Cu" "F.Mask")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/RF_GSM.3dshapes/Quectel_BC66.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
