(footprint "Quectel_BC95"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "GSM NB-IoT module, 19.9x23.6x2.2mm, https://www.quectel.com/UploadImage/Downlad/Quectel_BC95_Hardware_Design_V1.3.pdf")
	(tags "GSM NB-IoT module BC95")
	(property "Reference" "REF**"
		(at 0 -16.6 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(property "Value" "Quectel_BC95"
		(at 0 16.6 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" smd roundrect
		(at -10.1 -8.6)
		(size 2.6 0.6375)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at -10.1 -7.5)
		(size 2.6 0.6375)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at -10.1 -6.4)
		(size 2.6 0.6375)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at -10.1 -5.3)
		(size 2.6 0.6375)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at -10.1 -4.2)
		(size 2.6 0.6375)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at -10.1 -3.1)
		(size 2.6 0.6375)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at -10.1 -2)
		(size 2.6 0.6375)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at -10.1 -0.9)
		(size 2.6 0.6375)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at -10.1 0.2)
		(size 2.6 0.6375)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at -10.1 1.9)
		(size 2.6 0.6375)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at -10.1 3)
		(size 2.6 0.6375)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at -10.1 4.1)
		(size 2.6 0.6375)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at -10.1 5.2)
		(size 2.6 0.6375)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at -10.1 6.3)
		(size 2.6 0.6375)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at -10.1 7.4)
		(size 2.6 0.6375)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at -10.1 8.5)
		(size 2.6 0.6375)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at -6.35 -11.95 90)
		(size 2.6 0.6375)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at -6.35 11.95 90)
		(size 2.6 0.6375)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd circle
		(at -5.95 -4.25)
		(size 0.9 0.9)
		(layers "F.Paste")
	)
	(pad "" smd circle
		(at -5.95 -2.55)
		(size 0.9 0.9)
		(layers "F.Paste")
	)
	(pad "" smd circle
		(at -5.95 -0.85)
		(size 0.9 0.9)
		(layers "F.Paste")
	)
	(pad "" smd circle
		(at -5.95 0.85)
		(size 0.9 0.9)
		(layers "F.Paste")
	)
	(pad "" smd circle
		(at -5.95 2.55)
		(size 0.9 0.9)
		(layers "F.Paste")
	)
	(pad "" smd circle
		(at -5.95 4.25)
		(size 0.9 0.9)
		(layers "F.Paste")
	)
	(pad "" smd roundrect
		(at -5.25 -11.95 90)
		(size 2.6 0.6375)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at -5.25 11.95 90)
		(size 2.6 0.6375)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd circle
		(at -4.25 -4.25)
		(size 0.9 0.9)
		(layers "F.Paste")
	)
	(pad "" smd circle
		(at -4.25 -2.55)
		(size 0.9 0.9)
		(layers "F.Paste")
	)
	(pad "" smd circle
		(at -4.25 -0.85)
		(size 0.9 0.9)
		(layers "F.Paste")
	)
	(pad "" smd circle
		(at -4.25 0.85)
		(size 0.9 0.9)
		(layers "F.Paste")
	)
	(pad "" smd circle
		(at -4.25 2.55)
		(size 0.9 0.9)
		(layers "F.Paste")
	)
	(pad "" smd circle
		(at -4.25 4.25)
		(size 0.9 0.9)
		(layers "F.Paste")
	)
	(pad "" smd roundrect
		(at -4.15 -11.95 90)
		(size 2.6 0.6375)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at -4.15 11.95 90)
		(size 2.6 0.6375)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at -3.05 -11.95 90)
		(size 2.6 0.6375)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at -3.05 11.95 90)
		(size 2.6 0.6375)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd circle
		(at -2.55 -7.65)
		(size 0.9 0.9)
		(layers "F.Paste")
	)
	(pad "" smd circle
		(at -2.55 -5.95)
		(size 0.9 0.9)
		(layers "F.Paste")
	)
	(pad "" smd circle
		(at -2.55 5.95)
		(size 0.9 0.9)
		(layers "F.Paste")
	)
	(pad "" smd circle
		(at -2.55 7.65)
		(size 0.9 0.9)
		(layers "F.Paste")
	)
	(pad "" smd roundrect
		(at -1.95 -11.95 90)
		(size 2.6 0.6375)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at -1.95 11.95 90)
		(size 2.6 0.6375)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd circle
		(at -0.85 -7.65)
		(size 0.9 0.9)
		(layers "F.Paste")
	)
	(pad "" smd circle
		(at -0.85 -5.95)
		(size 0.9 0.9)
		(layers "F.Paste")
	)
	(pad "" smd circle
		(at -0.85 5.95)
		(size 0.9 0.9)
		(layers "F.Paste")
	)
	(pad "" smd circle
		(at -0.85 7.65)
		(size 0.9 0.9)
		(layers "F.Paste")
	)
	(pad "" smd roundrect
		(at 0.55 -11.95 90)
		(size 2.6 0.6375)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 0.55 11.95 90)
		(size 2.6 0.6375)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd circle
		(at 0.85 -7.65)
		(size 0.9 0.9)
		(layers "F.Paste")
	)
	(pad "" smd circle
		(at 0.85 -5.95)
		(size 0.9 0.9)
		(layers "F.Paste")
	)
	(pad "" smd circle
		(at 0.85 5.95)
		(size 0.9 0.9)
		(layers "F.Paste")
	)
	(pad "" smd circle
		(at 0.85 7.65)
		(size 0.9 0.9)
		(layers "F.Paste")
	)
	(pad "" smd roundrect
		(at 1.65 -11.95 90)
		(size 2.6 0.6375)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 1.65 11.95 90)
		(size 2.6 0.6375)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd circle
		(at 2.55 -7.65)
		(size 0.9 0.9)
		(layers "F.Paste")
	)
	(pad "" smd circle
		(at 2.55 -5.95)
		(size 0.9 0.9)
		(layers "F.Paste")
	)
	(pad "" smd circle
		(at 2.55 5.95)
		(size 0.9 0.9)
		(layers "F.Paste")
	)
	(pad "" smd circle
		(at 2.55 7.65)
		(size 0.9 0.9)
		(layers "F.Paste")
	)
	(pad "" smd roundrect
		(at 2.75 -11.95 90)
		(size 2.6 0.6375)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 2.75 11.95 90)
		(size 2.6 0.6375)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 3.85 -11.95 90)
		(size 2.6 0.6375)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 3.85 11.95 90)
		(size 2.6 0.6375)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd circle
		(at 4.25 -4.25)
		(size 0.9 0.9)
		(layers "F.Paste")
	)
	(pad "" smd circle
		(at 4.25 -2.55)
		(size 0.9 0.9)
		(layers "F.Paste")
	)
	(pad "" smd circle
		(at 4.25 -0.85)
		(size 0.9 0.9)
		(layers "F.Paste")
	)
	(pad "" smd circle
		(at 4.25 0.85)
		(size 0.9 0.9)
		(layers "F.Paste")
	)
	(pad "" smd circle
		(at 4.25 2.55)
		(size 0.9 0.9)
		(layers "F.Paste")
	)
	(pad "" smd circle
		(at 4.25 4.25)
		(size 0.9 0.9)
		(layers "F.Paste")
	)
	(pad "" smd roundrect
		(at 4.95 -11.95 90)
		(size 2.6 0.6375)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 4.95 11.95 90)
		(size 2.6 0.6375)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd circle
		(at 5.95 -4.25)
		(size 0.9 0.9)
		(layers "F.Paste")
	)
	(pad "" smd circle
		(at 5.95 -2.55)
		(size 0.9 0.9)
		(layers "F.Paste")
	)
	(pad "" smd circle
		(at 5.95 -0.85)
		(size 0.9 0.9)
		(layers "F.Paste")
	)
	(pad "" smd circle
		(at 5.95 0.85)
		(size 0.9 0.9)
		(layers "F.Paste")
	)
	(pad "" smd circle
		(at 5.95 2.55)
		(size 0.9 0.9)
		(layers "F.Paste")
	)
	(pad "" smd circle
		(at 5.95 4.25)
		(size 0.9 0.9)
		(layers "F.Paste")
	)
	(pad "" smd roundrect
		(at 6.05 -11.95 90)
		(size 2.6 0.6375)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 6.05 11.95 90)
		(size 2.6 0.6375)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 10.1 -8.6)
		(size 2.6 0.6375)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 10.1 -7.5)
		(size 2.6 0.6375)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 10.1 -6.4)
		(size 2.6 0.6375)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 10.1 -5.3)
		(size 2.6 0.6375)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 10.1 -4.2)
		(size 2.6 0.6375)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 10.1 -3.1)
		(size 2.6 0.6375)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 10.1 -2)
		(size 2.6 0.6375)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 10.1 -0.9)
		(size 2.6 0.6375)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 10.1 0.2)
		(size 2.6 0.6375)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 10.1 1.9)
		(size 2.6 0.6375)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 10.1 3)
		(size 2.6 0.6375)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 10.1 4.1)
		(size 2.6 0.6375)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 10.1 5.2)
		(size 2.6 0.6375)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 10.1 6.3)
		(size 2.6 0.6375)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 10.1 7.4)
		(size 2.6 0.6375)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 10.1 8.5)
		(size 2.6 0.6375)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "1" smd roundrect
		(at -9.8 -8.6)
		(size 2.4 0.75)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "2" smd roundrect
		(at -9.8 -7.5)
		(size 2.4 0.75)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "3" smd roundrect
		(at -9.8 -6.4)
		(size 2.4 0.75)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "4" smd roundrect
		(at -9.8 -5.3)
		(size 2.4 0.75)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "5" smd roundrect
		(at -9.8 -4.2)
		(size 2.4 0.75)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "6" smd roundrect
		(at -9.8 -3.1)
		(size 2.4 0.75)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "7" smd roundrect
		(at -9.8 -2)
		(size 2.4 0.75)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "8" smd roundrect
		(at -9.8 -0.9)
		(size 2.4 0.75)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "9" smd roundrect
		(at -9.8 0.2)
		(size 2.4 0.75)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "10" smd roundrect
		(at -9.8 1.9)
		(size 2.4 0.75)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "11" smd roundrect
		(at -9.8 3)
		(size 2.4 0.75)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "12" smd roundrect
		(at -9.8 4.1)
		(size 2.4 0.75)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "13" smd roundrect
		(at -9.8 5.2)
		(size 2.4 0.75)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "14" smd roundrect
		(at -9.8 6.3)
		(size 2.4 0.75)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "15" smd roundrect
		(at -9.8 7.4)
		(size 2.4 0.75)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "16" smd roundrect
		(at -9.8 8.5)
		(size 2.4 0.75)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "17" smd roundrect
		(at -6.35 11.65)
		(size 0.75 2.4)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "18" smd roundrect
		(at -5.25 11.65)
		(size 0.75 2.4)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "19" smd roundrect
		(at -4.15 11.65)
		(size 0.75 2.4)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "20" smd roundrect
		(at -3.05 11.65)
		(size 0.75 2.4)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "21" smd roundrect
		(at -1.95 11.65)
		(size 0.75 2.4)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "22" smd roundrect
		(at 0.55 11.65)
		(size 0.75 2.4)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "23" smd roundrect
		(at 1.65 11.65)
		(size 0.75 2.4)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "24" smd roundrect
		(at 2.75 11.65)
		(size 0.75 2.4)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "25" smd roundrect
		(at 3.85 11.65)
		(size 0.75 2.4)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "26" smd roundrect
		(at 4.95 11.65)
		(size 0.75 2.4)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "27" smd roundrect
		(at 6.05 11.65)
		(size 0.75 2.4)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "28" smd roundrect
		(at 9.8 8.5)
		(size 2.4 0.75)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "29" smd roundrect
		(at 9.8 7.4)
		(size 2.4 0.75)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "30" smd roundrect
		(at 9.8 6.3)
		(size 2.4 0.75)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "31" smd roundrect
		(at 9.8 5.2)
		(size 2.4 0.75)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "32" smd roundrect
		(at 9.8 4.1)
		(size 2.4 0.75)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "33" smd roundrect
		(at 9.8 3)
		(size 2.4 0.75)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "34" smd roundrect
		(at 9.8 1.9)
		(size 2.4 0.75)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "35" smd roundrect
		(at 9.8 0.2)
		(size 2.4 0.75)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "36" smd roundrect
		(at 9.8 -0.9)
		(size 2.4 0.75)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "37" smd roundrect
		(at 9.8 -2)
		(size 2.4 0.75)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "38" smd roundrect
		(at 9.8 -3.1)
		(size 2.4 0.75)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "39" smd roundrect
		(at 9.8 -4.2)
		(size 2.4 0.75)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "40" smd roundrect
		(at 9.8 -5.3)
		(size 2.4 0.75)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "41" smd roundrect
		(at 9.8 -6.4)
		(size 2.4 0.75)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "42" smd roundrect
		(at 9.8 -7.5)
		(size 2.4 0.75)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "43" smd roundrect
		(at 9.8 -8.6)
		(size 2.4 0.75)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "44" smd roundrect
		(at 6.05 -11.65)
		(size 0.75 2.4)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "45" smd roundrect
		(at 4.95 -11.65)
		(size 0.75 2.4)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "46" smd roundrect
		(at 3.85 -11.65)
		(size 0.75 2.4)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "47" smd roundrect
		(at 2.75 -11.65)
		(size 0.75 2.4)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "48" smd roundrect
		(at 1.65 -11.65)
		(size 0.75 2.4)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "49" smd roundrect
		(at 0.55 -11.65)
		(size 0.75 2.4)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "50" smd roundrect
		(at -1.95 -11.65)
		(size 0.75 2.4)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "51" smd roundrect
		(at -3.05 -11.65)
		(size 0.75 2.4)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "52" smd roundrect
		(at -4.15 -11.65)
		(size 0.75 2.4)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "53" smd roundrect
		(at -5.25 -11.65)
		(size 0.75 2.4)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "54" smd roundrect
		(at -6.35 -11.65)
		(size 0.75 2.4)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "55" smd rect
		(at -5.95 -4.25)
		(size 1 1)
		(layers "F.Cu" "F.Mask")
	)
	(pad "56" smd rect
		(at -5.95 -2.55)
		(size 1 1)
		(layers "F.Cu" "F.Mask")
	)
	(pad "57" smd rect
		(at -5.95 -0.85)
		(size 1 1)
		(layers "F.Cu" "F.Mask")
	)
	(pad "58" smd rect
		(at -5.95 0.85)
		(size 1 1)
		(layers "F.Cu" "F.Mask")
	)
	(pad "59" smd rect
		(at -5.95 2.55)
		(size 1 1)
		(layers "F.Cu" "F.Mask")
	)
	(pad "60" smd rect
		(at -5.95 4.25)
		(size 1 1)
		(layers "F.Cu" "F.Mask")
	)
	(pad "61" smd rect
		(at -2.55 7.65)
		(size 1 1)
		(layers "F.Cu" "F.Mask")
	)
	(pad "62" smd rect
		(at -0.85 7.65)
		(size 1 1)
		(layers "F.Cu" "F.Mask")
	)
	(pad "63" smd rect
		(at 0.85 7.65)
		(size 1 1)
		(layers "F.Cu" "F.Mask")
	)
	(pad "64" smd rect
		(at 2.55 7.65)
		(size 1 1)
		(layers "F.Cu" "F.Mask")
	)
	(pad "65" smd rect
		(at 5.95 4.25)
		(size 1 1)
		(layers "F.Cu" "F.Mask")
	)
	(pad "66" smd rect
		(at 5.95 2.55)
		(size 1 1)
		(layers "F.Cu" "F.Mask")
	)
	(pad "67" smd rect
		(at 5.95 0.85)
		(size 1 1)
		(layers "F.Cu" "F.Mask")
	)
	(pad "68" smd rect
		(at 5.95 -0.85)
		(size 1 1)
		(layers "F.Cu" "F.Mask")
	)
	(pad "69" smd rect
		(at 5.95 -2.55)
		(size 1 1)
		(layers "F.Cu" "F.Mask")
	)
	(pad "70" smd rect
		(at 5.95 -4.25)
		(size 1 1)
		(layers "F.Cu" "F.Mask")
	)
	(pad "71" smd rect
		(at 2.55 -7.65)
		(size 1 1)
		(layers "F.Cu" "F.Mask")
	)
	(pad "72" smd rect
		(at 0.85 -7.65)
		(size 1 1)
		(layers "F.Cu" "F.Mask")
	)
	(pad "73" smd rect
		(at -0.85 -7.65)
		(size 1 1)
		(layers "F.Cu" "F.Mask")
	)
	(pad "74" smd rect
		(at -2.55 -7.65)
		(size 1 1)
		(layers "F.Cu" "F.Mask")
	)
	(pad "75" smd rect
		(at -4.25 -4.25)
		(size 1 1)
		(layers "F.Cu" "F.Mask")
	)
	(pad "76" smd rect
		(at -4.25 -2.55)
		(size 1 1)
		(layers "F.Cu" "F.Mask")
	)
	(pad "77" smd rect
		(at -4.25 -0.85)
		(size 1 1)
		(layers "F.Cu" "F.Mask")
	)
	(pad "78" smd rect
		(at -4.25 0.85)
		(size 1 1)
		(layers "F.Cu" "F.Mask")
	)
	(pad "79" smd rect
		(at -4.25 2.55)
		(size 1 1)
		(layers "F.Cu" "F.Mask")
	)
	(pad "80" smd rect
		(at -4.25 4.25)
		(size 1 1)
		(layers "F.Cu" "F.Mask")
	)
	(pad "81" smd rect
		(at -2.55 5.95)
		(size 1 1)
		(layers "F.Cu" "F.Mask")
	)
	(pad "82" smd rect
		(at -0.85 5.95)
		(size 1 1)
		(layers "F.Cu" "F.Mask")
	)
	(pad "83" smd rect
		(at 0.85 5.95)
		(size 1 1)
		(layers "F.Cu" "F.Mask")
	)
	(pad "84" smd rect
		(at 2.55 5.95)
		(size 1 1)
		(layers "F.Cu" "F.Mask")
	)
	(pad "85" smd rect
		(at 4.25 4.25)
		(size 1 1)
		(layers "F.Cu" "F.Mask")
	)
	(pad "86" smd rect
		(at 4.25 2.55)
		(size 1 1)
		(layers "F.Cu" "F.Mask")
	)
	(pad "87" smd rect
		(at 4.25 0.85)
		(size 1 1)
		(layers "F.Cu" "F.Mask")
	)
	(pad "88" smd rect
		(at 4.25 -0.85)
		(size 1 1)
		(layers "F.Cu" "F.Mask")
	)
	(pad "89" smd rect
		(at 4.25 -2.55)
		(size 1 1)
		(layers "F.Cu" "F.Mask")
	)
	(pad "90" smd rect
		(at 4.25 -4.25)
		(size 1 1)
		(layers "F.Cu" "F.Mask")
	)
	(pad "91" smd rect
		(at 2.55 -5.95)
		(size 1 1)
		(layers "F.Cu" "F.Mask")
	)
	(pad "92" smd rect
		(at 0.85 -5.95)
		(size 1 1)
		(layers "F.Cu" "F.Mask")
	)
	(pad "93" smd rect
		(at -0.85 -5.95)
		(size 1 1)
		(layers "F.Cu" "F.Mask")
	)
	(pad "94" smd rect
		(at -2.55 -5.95)
		(size 1 1)
		(layers "F.Cu" "F.Mask")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/RF_GSM.3dshapes/Quectel_BC95.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
