(footprint "Quectel_M95"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Quad-Band GSM/GPRS module, 19.9x23.6x2.65mm, https://www.quectel.com/UploadImage/Downlad/M95_Hardware_Design_V1.3.pdf")
	(tags "GSM Module M95")
	(property "Reference" "REF**"
		(at 0 -16 0)
		(layer "F.SilkS")
	)
	(property "Value" "Quectel_M95"
		(at 0 16 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" smd oval
		(at -10.1 -7.5)
		(size 2.8 0.675)
		(layers "F.Paste")
	)
	(pad "" smd oval
		(at -10.1 -6.4)
		(size 2.8 0.675)
		(layers "F.Paste")
	)
	(pad "" smd oval
		(at -10.1 -5.3)
		(size 2.8 0.675)
		(layers "F.Paste")
	)
	(pad "" smd oval
		(at -10.1 -4.2)
		(size 2.8 0.675)
		(layers "F.Paste")
	)
	(pad "" smd oval
		(at -10.1 -3.1)
		(size 2.8 0.675)
		(layers "F.Paste")
	)
	(pad "" smd oval
		(at -10.1 1.9)
		(size 2.8 0.675)
		(layers "F.Paste")
	)
	(pad "" smd oval
		(at -10.1 3)
		(size 2.8 0.675)
		(layers "F.Paste")
	)
	(pad "" smd oval
		(at -10.1 4.1)
		(size 2.8 0.675)
		(layers "F.Paste")
	)
	(pad "" smd oval
		(at -10.1 5.2)
		(size 2.8 0.675)
		(layers "F.Paste")
	)
	(pad "" smd oval
		(at -10.1 6.3)
		(size 2.8 0.675)
		(layers "F.Paste")
	)
	(pad "" smd oval
		(at -10.1 7.4)
		(size 2.8 0.675)
		(layers "F.Paste")
	)
	(pad "" smd oval
		(at -6.35 -11.95)
		(size 0.675 2.8)
		(layers "F.Paste")
	)
	(pad "" smd oval
		(at -6.35 11.95)
		(size 0.675 2.8)
		(layers "F.Paste")
	)
	(pad "" smd oval
		(at -5.25 -11.95)
		(size 0.675 2.8)
		(layers "F.Paste")
	)
	(pad "" smd oval
		(at -5.25 11.95)
		(size 0.675 2.8)
		(layers "F.Paste")
	)
	(pad "" smd oval
		(at -4.15 -11.95)
		(size 0.675 2.8)
		(layers "F.Paste")
	)
	(pad "" smd oval
		(at -4.15 11.95)
		(size 0.675 2.8)
		(layers "F.Paste")
	)
	(pad "" smd oval
		(at -3.05 -11.95)
		(size 0.675 2.8)
		(layers "F.Paste")
	)
	(pad "" smd oval
		(at -3.05 11.95)
		(size 0.675 2.8)
		(layers "F.Paste")
	)
	(pad "" smd oval
		(at -1.35 11.95)
		(size 0.675 2.8)
		(layers "F.Paste")
	)
	(pad "" smd oval
		(at -0.05 11.95)
		(size 0.675 2.8)
		(layers "F.Paste")
	)
	(pad "" smd oval
		(at 1.65 -11.95)
		(size 0.675 2.8)
		(layers "F.Paste")
	)
	(pad "" smd oval
		(at 1.65 11.95)
		(size 0.675 2.8)
		(layers "F.Paste")
	)
	(pad "" smd oval
		(at 2.75 -11.95)
		(size 0.675 2.8)
		(layers "F.Paste")
	)
	(pad "" smd oval
		(at 2.75 11.95)
		(size 0.675 2.8)
		(layers "F.Paste")
	)
	(pad "" smd oval
		(at 3.85 -11.95)
		(size 0.675 2.8)
		(layers "F.Paste")
	)
	(pad "" smd oval
		(at 3.85 11.95)
		(size 0.675 2.8)
		(layers "F.Paste")
	)
	(pad "" smd oval
		(at 4.95 -11.95)
		(size 0.675 2.8)
		(layers "F.Paste")
	)
	(pad "" smd oval
		(at 4.95 11.95)
		(size 0.675 2.8)
		(layers "F.Paste")
	)
	(pad "" smd oval
		(at 6.05 -11.95)
		(size 0.675 2.8)
		(layers "F.Paste")
	)
	(pad "" smd oval
		(at 6.05 11.95)
		(size 0.675 2.8)
		(layers "F.Paste")
	)
	(pad "" smd oval
		(at 10.1 -7.5)
		(size 2.8 0.675)
		(layers "F.Paste")
	)
	(pad "" smd oval
		(at 10.1 -6.4)
		(size 2.8 0.675)
		(layers "F.Paste")
	)
	(pad "" smd oval
		(at 10.1 -5.3)
		(size 2.8 0.675)
		(layers "F.Paste")
	)
	(pad "" smd oval
		(at 10.1 -4.2)
		(size 2.8 0.675)
		(layers "F.Paste")
	)
	(pad "" smd oval
		(at 10.1 -3.1)
		(size 2.8 0.675)
		(layers "F.Paste")
	)
	(pad "" smd oval
		(at 10.1 1.9)
		(size 2.8 0.675)
		(layers "F.Paste")
	)
	(pad "" smd oval
		(at 10.1 3)
		(size 2.8 0.675)
		(layers "F.Paste")
	)
	(pad "" smd oval
		(at 10.1 4.1)
		(size 2.8 0.675)
		(layers "F.Paste")
	)
	(pad "" smd oval
		(at 10.1 5.2)
		(size 2.8 0.675)
		(layers "F.Paste")
	)
	(pad "" smd oval
		(at 10.1 6.3)
		(size 2.8 0.675)
		(layers "F.Paste")
	)
	(pad "" smd oval
		(at 10.1 7.4)
		(size 2.8 0.675)
		(layers "F.Paste")
	)
	(pad "1" smd oval
		(at -9.8 -7.5)
		(size 2.4 0.75)
		(layers "F.Cu" "F.Mask")
	)
	(pad "2" smd oval
		(at -9.8 -6.4)
		(size 2.4 0.75)
		(layers "F.Cu" "F.Mask")
	)
	(pad "3" smd oval
		(at -9.8 -5.3)
		(size 2.4 0.75)
		(layers "F.Cu" "F.Mask")
	)
	(pad "4" smd oval
		(at -9.8 -4.2)
		(size 2.4 0.75)
		(layers "F.Cu" "F.Mask")
	)
	(pad "5" smd oval
		(at -9.8 -3.1)
		(size 2.4 0.75)
		(layers "F.Cu" "F.Mask")
	)
	(pad "6" smd oval
		(at -9.8 1.9)
		(size 2.4 0.75)
		(layers "F.Cu" "F.Mask")
	)
	(pad "7" smd oval
		(at -9.8 3)
		(size 2.4 0.75)
		(layers "F.Cu" "F.Mask")
	)
	(pad "8" smd oval
		(at -9.8 4.1)
		(size 2.4 0.75)
		(layers "F.Cu" "F.Mask")
	)
	(pad "9" smd oval
		(at -9.8 5.2)
		(size 2.4 0.75)
		(layers "F.Cu" "F.Mask")
	)
	(pad "10" smd oval
		(at -9.8 6.3)
		(size 2.4 0.75)
		(layers "F.Cu" "F.Mask")
	)
	(pad "11" smd oval
		(at -9.8 7.4)
		(size 2.4 0.75)
		(layers "F.Cu" "F.Mask")
	)
	(pad "12" smd oval
		(at -6.35 11.65)
		(size 0.75 2.4)
		(layers "F.Cu" "F.Mask")
	)
	(pad "13" smd oval
		(at -5.25 11.65)
		(size 0.75 2.4)
		(layers "F.Cu" "F.Mask")
	)
	(pad "14" smd oval
		(at -4.15 11.65)
		(size 0.75 2.4)
		(layers "F.Cu" "F.Mask")
	)
	(pad "15" smd oval
		(at -3.05 11.65)
		(size 0.75 2.4)
		(layers "F.Cu" "F.Mask")
	)
	(pad "16" smd oval
		(at 1.65 11.65)
		(size 0.75 2.4)
		(layers "F.Cu" "F.Mask")
	)
	(pad "17" smd oval
		(at 2.75 11.65)
		(size 0.75 2.4)
		(layers "F.Cu" "F.Mask")
	)
	(pad "18" smd oval
		(at 3.85 11.65)
		(size 0.75 2.4)
		(layers "F.Cu" "F.Mask")
	)
	(pad "19" smd oval
		(at 4.95 11.65)
		(size 0.75 2.4)
		(layers "F.Cu" "F.Mask")
	)
	(pad "20" smd oval
		(at 6.05 11.65)
		(size 0.75 2.4)
		(layers "F.Cu" "F.Mask")
	)
	(pad "21" smd oval
		(at 9.8 7.4)
		(size 2.4 0.75)
		(layers "F.Cu" "F.Mask")
	)
	(pad "22" smd oval
		(at 9.8 6.3)
		(size 2.4 0.75)
		(layers "F.Cu" "F.Mask")
	)
	(pad "23" smd oval
		(at 9.8 5.2)
		(size 2.4 0.75)
		(layers "F.Cu" "F.Mask")
	)
	(pad "24" smd oval
		(at 9.8 4.1)
		(size 2.4 0.75)
		(layers "F.Cu" "F.Mask")
	)
	(pad "25" smd oval
		(at 9.8 3)
		(size 2.4 0.75)
		(layers "F.Cu" "F.Mask")
	)
	(pad "26" smd oval
		(at 9.8 1.9)
		(size 2.4 0.75)
		(layers "F.Cu" "F.Mask")
	)
	(pad "27" smd oval
		(at 9.8 -3.1)
		(size 2.4 0.75)
		(layers "F.Cu" "F.Mask")
	)
	(pad "28" smd oval
		(at 9.8 -4.2)
		(size 2.4 0.75)
		(layers "F.Cu" "F.Mask")
	)
	(pad "29" smd oval
		(at 9.8 -5.3)
		(size 2.4 0.75)
		(layers "F.Cu" "F.Mask")
	)
	(pad "30" smd oval
		(at 9.8 -6.4)
		(size 2.4 0.75)
		(layers "F.Cu" "F.Mask")
	)
	(pad "31" smd oval
		(at 9.8 -7.5)
		(size 2.4 0.75)
		(layers "F.Cu" "F.Mask")
	)
	(pad "32" smd oval
		(at 6.05 -11.65)
		(size 0.75 2.4)
		(layers "F.Cu" "F.Mask")
	)
	(pad "33" smd oval
		(at 4.95 -11.65)
		(size 0.75 2.4)
		(layers "F.Cu" "F.Mask")
	)
	(pad "34" smd oval
		(at 3.85 -11.65)
		(size 0.75 2.4)
		(layers "F.Cu" "F.Mask")
	)
	(pad "35" smd oval
		(at 2.75 -11.65)
		(size 0.75 2.4)
		(layers "F.Cu" "F.Mask")
	)
	(pad "36" smd oval
		(at 1.65 -11.65)
		(size 0.75 2.4)
		(layers "F.Cu" "F.Mask")
	)
	(pad "37" smd oval
		(at -3.05 -11.65)
		(size 0.75 2.4)
		(layers "F.Cu" "F.Mask")
	)
	(pad "38" smd oval
		(at -4.15 -11.65)
		(size 0.75 2.4)
		(layers "F.Cu" "F.Mask")
	)
	(pad "39" smd oval
		(at -5.25 -11.65)
		(size 0.75 2.4)
		(layers "F.Cu" "F.Mask")
	)
	(pad "40" smd oval
		(at -6.35 -11.65)
		(size 0.75 2.4)
		(layers "F.Cu" "F.Mask")
	)
	(pad "41" smd oval
		(at -1.35 11.65)
		(size 0.75 2.4)
		(layers "F.Cu" "F.Mask")
	)
	(pad "42" smd oval
		(at -0.05 11.65)
		(size 0.75 2.4)
		(layers "F.Cu" "F.Mask")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/RF_GSM.3dshapes/Quectel_M95.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
