(footprint "SIMCom_SIM800C"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Quad-Band GSM/GPRS module, 17.6x15.7x2.3mm, http://simcom.ee/documents/SIM800C/SIM800C_Hardware_Design_V1.05.pdf")
	(tags "GSM Module SIM800C")
	(property "Reference" "REF**"
		(at 0 -11 0)
		(layer "F.SilkS")
	)
	(property "Value" "SIMCom_SIM800C"
		(at 0 11 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "of Area"
		(at 6 -4.97 90)
		(layer "Cmts.User")
	)
	(fp_text user "Keep out "
		(at 5.18 -4.95 90)
		(layer "Cmts.User")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" smd oval
		(at -7.95 -6.05)
		(size 1.8 0.55)
		(layers "F.Paste")
	)
	(pad "" smd oval
		(at -7.95 -4.95)
		(size 1.8 0.55)
		(layers "F.Paste")
	)
	(pad "" smd oval
		(at -7.95 -3.85)
		(size 1.8 0.55)
		(layers "F.Paste")
	)
	(pad "" smd oval
		(at -7.95 -2.75)
		(size 1.8 0.55)
		(layers "F.Paste")
	)
	(pad "" smd oval
		(at -7.95 -1.65)
		(size 1.8 0.55)
		(layers "F.Paste")
	)
	(pad "" smd oval
		(at -7.95 -0.55)
		(size 1.8 0.55)
		(layers "F.Paste")
	)
	(pad "" smd oval
		(at -7.95 0.55)
		(size 1.8 0.55)
		(layers "F.Paste")
	)
	(pad "" smd oval
		(at -7.95 1.65)
		(size 1.8 0.55)
		(layers "F.Paste")
	)
	(pad "" smd oval
		(at -7.95 2.75)
		(size 1.8 0.55)
		(layers "F.Paste")
	)
	(pad "" smd oval
		(at -7.95 3.85)
		(size 1.8 0.55)
		(layers "F.Paste")
	)
	(pad "" smd oval
		(at -7.95 4.95)
		(size 1.8 0.55)
		(layers "F.Paste")
	)
	(pad "" smd oval
		(at -7.95 6.05)
		(size 1.8 0.55)
		(layers "F.Paste")
	)
	(pad "" smd oval
		(at -4.4 -8.9 90)
		(size 1.8 0.55)
		(layers "F.Paste")
	)
	(pad "" smd oval
		(at -4.4 8.9 90)
		(size 1.8 0.55)
		(layers "F.Paste")
	)
	(pad "" smd oval
		(at -3.3 -8.9 90)
		(size 1.8 0.55)
		(layers "F.Paste")
	)
	(pad "" smd oval
		(at -3.3 8.9 90)
		(size 1.8 0.55)
		(layers "F.Paste")
	)
	(pad "" smd oval
		(at -2.2 -8.9 90)
		(size 1.8 0.55)
		(layers "F.Paste")
	)
	(pad "" smd oval
		(at -2.2 8.9 90)
		(size 1.8 0.55)
		(layers "F.Paste")
	)
	(pad "" smd oval
		(at -1.1 -8.9 90)
		(size 1.8 0.55)
		(layers "F.Paste")
	)
	(pad "" smd oval
		(at -1.1 8.9 90)
		(size 1.8 0.55)
		(layers "F.Paste")
	)
	(pad "" smd oval
		(at 0 -8.9 90)
		(size 1.8 0.55)
		(layers "F.Paste")
	)
	(pad "" smd oval
		(at 0 8.9 90)
		(size 1.8 0.55)
		(layers "F.Paste")
	)
	(pad "" smd oval
		(at 1.1 -8.9 90)
		(size 1.8 0.55)
		(layers "F.Paste")
	)
	(pad "" smd oval
		(at 1.1 8.9 90)
		(size 1.8 0.55)
		(layers "F.Paste")
	)
	(pad "" smd oval
		(at 2.2 -8.9 90)
		(size 1.8 0.55)
		(layers "F.Paste")
	)
	(pad "" smd oval
		(at 2.2 8.9 90)
		(size 1.8 0.55)
		(layers "F.Paste")
	)
	(pad "" smd oval
		(at 3.3 -8.9 90)
		(size 1.8 0.55)
		(layers "F.Paste")
	)
	(pad "" smd oval
		(at 3.3 8.9 90)
		(size 1.8 0.55)
		(layers "F.Paste")
	)
	(pad "" smd oval
		(at 4.4 -8.9 90)
		(size 1.8 0.55)
		(layers "F.Paste")
	)
	(pad "" smd oval
		(at 4.4 8.9 90)
		(size 1.8 0.55)
		(layers "F.Paste")
	)
	(pad "" smd oval
		(at 7.95 -6.05)
		(size 1.8 0.55)
		(layers "F.Paste")
	)
	(pad "" smd oval
		(at 7.95 -4.95)
		(size 1.8 0.55)
		(layers "F.Paste")
	)
	(pad "" smd oval
		(at 7.95 -3.85)
		(size 1.8 0.55)
		(layers "F.Paste")
	)
	(pad "" smd oval
		(at 7.95 -2.75)
		(size 1.8 0.55)
		(layers "F.Paste")
	)
	(pad "" smd oval
		(at 7.95 -1.65)
		(size 1.8 0.55)
		(layers "F.Paste")
	)
	(pad "" smd oval
		(at 7.95 -0.55)
		(size 1.8 0.55)
		(layers "F.Paste")
	)
	(pad "" smd oval
		(at 7.95 0.55)
		(size 1.8 0.55)
		(layers "F.Paste")
	)
	(pad "" smd oval
		(at 7.95 1.65)
		(size 1.8 0.55)
		(layers "F.Paste")
	)
	(pad "" smd oval
		(at 7.95 2.75)
		(size 1.8 0.55)
		(layers "F.Paste")
	)
	(pad "" smd oval
		(at 7.95 3.85)
		(size 1.8 0.55)
		(layers "F.Paste")
	)
	(pad "" smd oval
		(at 7.95 4.95)
		(size 1.8 0.55)
		(layers "F.Paste")
	)
	(pad "" smd oval
		(at 7.95 6.05)
		(size 1.8 0.55)
		(layers "F.Paste")
	)
	(pad "1" smd oval
		(at -7.85 -6.05)
		(size 1.6 0.6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "2" smd oval
		(at -7.85 -4.95)
		(size 1.6 0.6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "3" smd oval
		(at -7.85 -3.85)
		(size 1.6 0.6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "4" smd oval
		(at -7.85 -2.75)
		(size 1.6 0.6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "5" smd oval
		(at -7.85 -1.65)
		(size 1.6 0.6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "6" smd oval
		(at -7.85 -0.55)
		(size 1.6 0.6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "7" smd oval
		(at -7.85 0.55)
		(size 1.6 0.6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "8" smd oval
		(at -7.85 1.65)
		(size 1.6 0.6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "9" smd oval
		(at -7.85 2.75)
		(size 1.6 0.6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "10" smd oval
		(at -7.85 3.85)
		(size 1.6 0.6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "11" smd oval
		(at -7.85 4.95)
		(size 1.6 0.6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "12" smd oval
		(at -7.85 6.05)
		(size 1.6 0.6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "13" smd oval
		(at -4.4 8.8)
		(size 0.6 1.6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "14" smd oval
		(at -3.3 8.8)
		(size 0.6 1.6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "15" smd oval
		(at -2.2 8.8)
		(size 0.6 1.6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "16" smd oval
		(at -1.1 8.8)
		(size 0.6 1.6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "17" smd oval
		(at 0 8.8)
		(size 0.6 1.6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "18" smd oval
		(at 1.1 8.8)
		(size 0.6 1.6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "19" smd oval
		(at 2.2 8.8)
		(size 0.6 1.6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "20" smd oval
		(at 3.3 8.8)
		(size 0.6 1.6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "21" smd oval
		(at 4.4 8.8)
		(size 0.6 1.6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "22" smd oval
		(at 7.85 6.05)
		(size 1.6 0.6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "23" smd oval
		(at 7.85 4.95)
		(size 1.6 0.6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "24" smd oval
		(at 7.85 3.85)
		(size 1.6 0.6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "25" smd oval
		(at 7.85 2.75)
		(size 1.6 0.6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "26" smd oval
		(at 7.85 1.65)
		(size 1.6 0.6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "27" smd oval
		(at 7.85 0.55)
		(size 1.6 0.6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "28" smd oval
		(at 7.85 -0.55)
		(size 1.6 0.6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "29" smd oval
		(at 7.85 -1.65)
		(size 1.6 0.6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "30" smd oval
		(at 7.85 -2.75)
		(size 1.6 0.6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "31" smd oval
		(at 7.85 -3.85)
		(size 1.6 0.6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "32" smd oval
		(at 7.85 -4.95)
		(size 1.6 0.6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "33" smd oval
		(at 7.85 -6.05)
		(size 1.6 0.6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "34" smd oval
		(at 4.4 -8.8)
		(size 0.6 1.6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "35" smd oval
		(at 3.3 -8.8)
		(size 0.6 1.6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "36" smd oval
		(at 2.2 -8.8)
		(size 0.6 1.6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "37" smd oval
		(at 1.1 -8.8)
		(size 0.6 1.6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "38" smd oval
		(at 0 -8.8)
		(size 0.6 1.6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "39" smd oval
		(at -1.1 -8.8)
		(size 0.6 1.6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "40" smd oval
		(at -2.2 -8.8)
		(size 0.6 1.6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "41" smd oval
		(at -3.3 -8.8)
		(size 0.6 1.6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "42" smd oval
		(at -4.4 -8.8)
		(size 0.6 1.6)
		(layers "F.Cu" "F.Mask")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/RF_GSM.3dshapes/SIMCom_SIM800C.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
