(footprint "SIMCom_SIM900"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Quad-Band GSM/GPRS module, 24x24x3mm, http://simcom.ee/documents/SIM900/SIM900_Hardware%20Design_V2.05.pdf")
	(tags "GSM Module SIM900")
	(property "Reference" "REF**"
		(at 0 -14 0)
		(layer "F.SilkS")
	)
	(property "Value" "SIMCom_SIM900"
		(at 0 4 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "Area"
		(at -0.5 -8.3 0)
		(layer "Cmts.User")
	)
	(fp_text user "A"
		(at -0.5 -7.5 0)
		(layer "Cmts.User")
	)
	(fp_text user "type of copper"
		(at -0.5 -5.5 0)
		(layer "Cmts.User")
	)
	(fp_text user "Keepout any"
		(at -0.5 -6.5 0)
		(layer "Cmts.User")
	)
	(fp_text user "Keepout vias"
		(at -4.4 -0.7 0)
		(layer "Cmts.User")
	)
	(fp_text user "Area B"
		(at -4.5974 -2.0828 0)
		(layer "Cmts.User")
	)
	(fp_text user "${REFERENCE}"
		(at 0 5.5 0)
		(layer "F.Fab")
	)
	(pad "1" smd oval
		(at -12 -8)
		(size 1.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd oval
		(at -12 -7)
		(size 1.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd oval
		(at -12 -6)
		(size 1.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd oval
		(at -12 -5)
		(size 1.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd oval
		(at -12 -4)
		(size 1.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd oval
		(at -12 -3)
		(size 1.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd oval
		(at -12 -2)
		(size 1.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd oval
		(at -12 -1)
		(size 1.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd oval
		(at -12 0)
		(size 1.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd oval
		(at -12 1)
		(size 1.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd oval
		(at -12 2)
		(size 1.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "12" smd oval
		(at -12 3)
		(size 1.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "13" smd oval
		(at -12 4)
		(size 1.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "14" smd oval
		(at -12 5)
		(size 1.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "15" smd oval
		(at -12 6)
		(size 1.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "16" smd oval
		(at -12 7)
		(size 1.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "17" smd oval
		(at -12 8)
		(size 1.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "18" smd oval
		(at -8 12)
		(size 0.6 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "19" smd oval
		(at -7 12)
		(size 0.6 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "20" smd oval
		(at -6 12)
		(size 0.6 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "21" smd oval
		(at -5 12)
		(size 0.6 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "22" smd oval
		(at -4 12)
		(size 0.6 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "23" smd oval
		(at -3 12)
		(size 0.6 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "24" smd oval
		(at -2 12)
		(size 0.6 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "25" smd oval
		(at -1 12)
		(size 0.6 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "26" smd oval
		(at 0 12)
		(size 0.6 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "27" smd oval
		(at 1 12)
		(size 0.6 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "28" smd oval
		(at 2 12)
		(size 0.6 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "29" smd oval
		(at 3 12)
		(size 0.6 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "30" smd oval
		(at 4 12)
		(size 0.6 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "31" smd oval
		(at 5 12)
		(size 0.6 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "32" smd oval
		(at 6 12)
		(size 0.6 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "33" smd oval
		(at 7 12)
		(size 0.6 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "34" smd oval
		(at 8 12)
		(size 0.6 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "35" smd oval
		(at 12 8)
		(size 1.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "36" smd oval
		(at 12 7)
		(size 1.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "37" smd oval
		(at 12 6)
		(size 1.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "38" smd oval
		(at 12 5)
		(size 1.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "39" smd oval
		(at 12 4)
		(size 1.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "40" smd oval
		(at 12 3)
		(size 1.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "41" smd oval
		(at 12 2)
		(size 1.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "42" smd oval
		(at 12 1)
		(size 1.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "43" smd oval
		(at 12 0)
		(size 1.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "44" smd oval
		(at 12 -1)
		(size 1.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "45" smd oval
		(at 12 -2)
		(size 1.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "46" smd oval
		(at 12 -3)
		(size 1.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "47" smd oval
		(at 12 -4)
		(size 1.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "48" smd oval
		(at 12 -5)
		(size 1.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "49" smd oval
		(at 12 -6)
		(size 1.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "50" smd oval
		(at 12 -7)
		(size 1.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "51" smd oval
		(at 12 -8)
		(size 1.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "52" smd oval
		(at 8 -12)
		(size 0.6 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "53" smd oval
		(at 7 -12)
		(size 0.6 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "54" smd oval
		(at 6 -12)
		(size 0.6 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "55" smd oval
		(at 5 -12)
		(size 0.6 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "56" smd oval
		(at 4 -12)
		(size 0.6 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "57" smd oval
		(at 3 -12)
		(size 0.6 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "58" smd oval
		(at 2 -12)
		(size 0.6 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "59" smd oval
		(at 1 -12)
		(size 0.6 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "60" smd oval
		(at 0 -12)
		(size 0.6 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "61" smd oval
		(at -1 -12)
		(size 0.6 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "62" smd oval
		(at -2 -12)
		(size 0.6 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "63" smd oval
		(at -3 -12)
		(size 0.6 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "64" smd oval
		(at -4 -12)
		(size 0.6 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "65" smd oval
		(at -5 -12)
		(size 0.6 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "66" smd oval
		(at -6 -12)
		(size 0.6 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "67" smd oval
		(at -7 -12)
		(size 0.6 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "68" smd oval
		(at -8 -12)
		(size 0.6 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(hatch full 0.508)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy -7.3 -2.8) (xy -1.7 -2.8) (xy -1.7 2.8) (xy -7.3 2.8)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(hatch full 0.508)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints not_allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy 0.504839 -8) (xy 0.485702 -8.195174) (xy 0.42902 -8.382914) (xy 0.336952 -8.556069) (xy 0.213004 -8.708044)
				(xy 0.061899 -8.833049) (xy -0.110609 -8.926324) (xy -0.297949 -8.984315) (xy -0.492985 -9.004815)
				(xy -0.688288 -8.987041) (xy -0.876419 -8.93167) (xy -1.050213 -8.840813) (xy -1.203049 -8.71793)
				(xy -1.329106 -8.567701) (xy -1.423583 -8.395848) (xy -1.482881 -8.208918) (xy -1.504741 -8.01403)
				(xy -1.488331 -7.818607) (xy -1.434276 -7.630094) (xy -1.344634 -7.45567) (xy -1.222821 -7.30198)
				(xy -1.073475 -7.174877) (xy -0.902286 -7.079203) (xy -0.715774 -7.018602) (xy -0.521044 -6.995381)
				(xy -0.325512 -7.010427) (xy -0.136626 -7.063165) (xy 0.03842 -7.151586) (xy 0.192957 -7.272324)
				(xy 0.321099 -7.420778) (xy 0.417966 -7.591295) (xy 0.479868 -7.777379) (xy 0.504447 -7.971943)
			)
		)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/RF_GSM.3dshapes/SIMCom_SIM900.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
