(footprint "Telit_SE150A4"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Telit SE150A4 smart module, https://atoma.spb.ru/sites/default/files/documents/telit_se150a4_smart_module_hardware_user_guide_r1.pdf")
	(tags "Smart module Telit SE150")
	(property "Reference" "REF**"
		(at 0 -22.5 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(property "Value" "Telit_SE150A4"
		(at 0 2 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(pad "" smd roundrect
		(at -13.85 -10.85 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at -13.85 -10.15 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at -13.85 -7.85 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at -13.85 -7.15 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at -13.85 -4.85 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at -13.85 -4.15 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at -13.85 -1.85 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at -13.85 -1.15 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at -13.85 1.15 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at -13.85 1.85 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at -13.85 4.15 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at -13.85 4.85 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at -13.85 7.15 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at -13.85 7.85 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at -13.85 10.15 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at -13.85 10.85 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at -13.15 -10.85 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at -13.15 -10.15 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at -13.15 -7.85 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at -13.15 -7.15 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at -13.15 -4.85 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at -13.15 -4.15 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at -13.15 -1.85 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at -13.15 -1.15 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at -13.15 1.15 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at -13.15 1.85 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at -13.15 4.15 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at -13.15 4.85 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at -13.15 7.15 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at -13.15 7.85 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at -13.15 10.15 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at -13.15 10.85 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at -10.85 -13.85 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at -10.85 -13.15 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at -10.85 -4.85 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at -10.85 -4.15 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at -10.85 -1.85 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at -10.85 -1.15 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at -10.85 1.15 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at -10.85 1.85 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at -10.85 4.15 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at -10.85 4.85 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at -10.85 13.15 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at -10.85 13.85 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at -10.15 -13.85 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at -10.15 -13.15 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at -10.15 -4.85 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at -10.15 -4.15 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at -10.15 -1.85 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at -10.15 -1.15 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at -10.15 1.15 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at -10.15 1.85 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at -10.15 4.15 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at -10.15 4.85 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at -10.15 13.15 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at -10.15 13.85 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at -7.85 -13.85 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at -7.85 -13.15 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at -7.85 -4.85 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at -7.85 -4.15 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at -7.85 -1.85 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at -7.85 -1.15 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at -7.85 1.15 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at -7.85 1.85 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at -7.85 4.15 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at -7.85 4.85 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at -7.85 13.15 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at -7.85 13.85 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at -7.15 -13.85 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at -7.15 -13.15 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at -7.15 -4.85 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at -7.15 -4.15 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at -7.15 -1.85 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at -7.15 -1.15 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at -7.15 1.15 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at -7.15 1.85 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at -7.15 4.15 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at -7.15 4.85 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at -7.15 13.15 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at -7.15 13.85 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at -4.85 -13.85 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at -4.85 -13.15 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at -4.85 -10.85 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at -4.85 -10.15 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at -4.85 -7.85 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at -4.85 -7.15 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at -4.85 7.15 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at -4.85 7.85 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at -4.85 10.15 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at -4.85 10.85 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at -4.85 13.15 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at -4.85 13.85 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at -4.15 -13.85 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at -4.15 -13.15 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at -4.15 -10.85 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at -4.15 -10.15 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at -4.15 -7.85 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at -4.15 -7.15 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at -4.15 7.15 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at -4.15 7.85 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at -4.15 10.15 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at -4.15 10.85 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at -4.15 13.15 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at -4.15 13.85 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at -1.85 -13.85 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at -1.85 -13.15 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at -1.85 -10.85 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at -1.85 -10.15 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at -1.85 -7.85 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at -1.85 -7.15 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at -1.85 7.15 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at -1.85 7.85 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at -1.85 10.15 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at -1.85 10.85 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at -1.85 13.15 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at -1.85 13.85 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at -1.15 -13.85 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at -1.15 -13.15 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at -1.15 -10.85 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at -1.15 -10.15 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at -1.15 -7.85 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at -1.15 -7.15 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at -1.15 7.15 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at -1.15 7.85 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at -1.15 10.15 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at -1.15 10.85 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at -1.15 13.15 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at -1.15 13.85 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at 1.15 -13.85 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at 1.15 -13.15 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at 1.15 -10.85 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at 1.15 -10.15 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at 1.15 -7.85 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at 1.15 -7.15 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at 1.15 7.15 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at 1.15 7.85 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at 1.15 10.15 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at 1.15 10.85 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at 1.15 13.15 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at 1.15 13.85 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at 1.85 -13.85 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at 1.85 -13.15 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at 1.85 -10.85 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at 1.85 -10.15 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at 1.85 -7.85 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at 1.85 -7.15 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at 1.85 7.15 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at 1.85 7.85 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at 1.85 10.15 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at 1.85 10.85 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at 1.85 13.15 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at 1.85 13.85 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at 4.15 -13.85 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at 4.15 -13.15 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at 4.15 -10.85 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at 4.15 -10.15 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at 4.15 -7.85 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at 4.15 -7.15 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at 4.15 7.15 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at 4.15 7.85 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at 4.15 10.15 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at 4.15 10.85 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at 4.15 13.15 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at 4.15 13.85 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at 4.85 -13.85 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at 4.85 -13.15 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at 4.85 -10.85 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at 4.85 -10.15 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at 4.85 -7.85 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at 4.85 -7.15 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at 4.85 7.15 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at 4.85 7.85 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at 4.85 10.15 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at 4.85 10.85 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at 4.85 13.15 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at 4.85 13.85 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at 7.15 -13.85 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at 7.15 -13.15 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at 7.15 -4.85 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at 7.15 -4.15 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at 7.15 -1.85 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at 7.15 -1.15 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at 7.15 1.15 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at 7.15 1.85 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at 7.15 4.15 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at 7.15 4.85 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at 7.15 13.15 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at 7.15 13.85 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at 7.85 -13.85 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at 7.85 -13.15 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at 7.85 -4.85 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at 7.85 -4.15 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at 7.85 -1.85 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at 7.85 -1.15 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at 7.85 1.15 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at 7.85 1.85 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at 7.85 4.15 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at 7.85 4.85 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at 7.85 13.15 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at 7.85 13.85 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at 10.15 -13.85 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at 10.15 -13.15 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at 10.15 -4.85 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at 10.15 -4.15 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at 10.15 -1.85 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at 10.15 -1.15 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at 10.15 1.15 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at 10.15 1.85 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at 10.15 4.15 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at 10.15 4.85 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at 10.15 13.15 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at 10.15 13.85 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at 10.85 -13.85 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at 10.85 -13.15 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at 10.85 -4.85 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at 10.85 -4.15 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at 10.85 -1.85 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at 10.85 -1.15 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at 10.85 1.15 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at 10.85 1.85 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at 10.85 4.15 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at 10.85 4.85 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at 10.85 13.15 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at 10.85 13.85 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at 13.15 -10.85 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at 13.15 -10.15 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at 13.15 -7.85 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at 13.15 -7.15 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at 13.15 -4.85 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at 13.15 -4.15 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at 13.15 -1.85 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at 13.15 -1.15 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at 13.15 1.15 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at 13.15 1.85 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at 13.15 4.15 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at 13.15 4.85 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at 13.15 7.15 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at 13.15 7.85 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at 13.15 10.15 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at 13.15 10.85 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at 13.85 -10.85 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at 13.85 -10.15 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at 13.85 -7.85 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at 13.85 -7.15 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at 13.85 -4.85 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at 13.85 -4.15 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at 13.85 -1.85 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at 13.85 -1.15 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at 13.85 1.15 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at 13.85 1.85 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at 13.85 4.15 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at 13.85 4.85 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at 13.85 7.15 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at 13.85 7.85 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at 13.85 10.15 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at 13.85 10.85 90)
		(size 0.6 0.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "1" smd roundrect
		(at -20.15 -18)
		(size 2.2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "2" smd roundrect
		(at -20.15 -17)
		(size 2.2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "3" smd roundrect
		(at -20.15 -16)
		(size 2.2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "4" smd roundrect
		(at -20.15 -15)
		(size 2.2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "5" smd roundrect
		(at -20.15 -14)
		(size 2.2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "6" smd roundrect
		(at -20.15 -13)
		(size 2.2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "7" smd roundrect
		(at -20.15 -12)
		(size 2.2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "8" smd roundrect
		(at -20.15 -11)
		(size 2.2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "9" smd roundrect
		(at -20.15 -10)
		(size 2.2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "10" smd roundrect
		(at -20.15 -9)
		(size 2.2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "11" smd roundrect
		(at -20.15 -8)
		(size 2.2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "12" smd roundrect
		(at -20.15 -7)
		(size 2.2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "13" smd roundrect
		(at -20.15 -6)
		(size 2.2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "14" smd roundrect
		(at -20.15 -5)
		(size 2.2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "15" smd roundrect
		(at -20.15 -4)
		(size 2.2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "16" smd roundrect
		(at -20.15 -3)
		(size 2.2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "17" smd roundrect
		(at -20.15 -2)
		(size 2.2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "18" smd roundrect
		(at -20.15 -1)
		(size 2.2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "19" smd roundrect
		(at -20.15 0)
		(size 2.2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "20" smd roundrect
		(at -20.15 1)
		(size 2.2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "21" smd roundrect
		(at -20.15 2)
		(size 2.2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "22" smd roundrect
		(at -20.15 3)
		(size 2.2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "23" smd roundrect
		(at -20.15 4)
		(size 2.2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "24" smd roundrect
		(at -20.15 5)
		(size 2.2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "25" smd roundrect
		(at -20.15 6)
		(size 2.2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "26" smd roundrect
		(at -20.15 7)
		(size 2.2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "27" smd roundrect
		(at -20.15 8)
		(size 2.2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "28" smd roundrect
		(at -20.15 9)
		(size 2.2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "29" smd roundrect
		(at -20.15 10)
		(size 2.2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "30" smd roundrect
		(at -20.15 11)
		(size 2.2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "31" smd roundrect
		(at -20.15 12)
		(size 2.2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "32" smd roundrect
		(at -20.15 13)
		(size 2.2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "33" smd roundrect
		(at -20.15 14)
		(size 2.2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "34" smd roundrect
		(at -20.15 15)
		(size 2.2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "35" smd roundrect
		(at -20.15 16)
		(size 2.2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "36" smd roundrect
		(at -20.15 17)
		(size 2.2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "37" smd roundrect
		(at -20.15 18)
		(size 2.2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "38" smd roundrect
		(at -17.5 20.15 90)
		(size 2.2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "39" smd roundrect
		(at -16.5 20.15 90)
		(size 2.2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "40" smd roundrect
		(at -15.5 20.15 90)
		(size 2.2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "41" smd roundrect
		(at -14.5 20.15 90)
		(size 2.2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "42" smd roundrect
		(at -13.5 20.15 90)
		(size 2.2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "43" smd roundrect
		(at -12.5 20.15 90)
		(size 2.2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "44" smd roundrect
		(at -11.5 20.15 90)
		(size 2.2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "45" smd roundrect
		(at -10.5 20.15 90)
		(size 2.2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "46" smd roundrect
		(at -9.5 20.15 90)
		(size 2.2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "47" smd roundrect
		(at -8.5 20.15 90)
		(size 2.2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "48" smd roundrect
		(at -7.5 20.15 90)
		(size 2.2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "49" smd roundrect
		(at -6.5 20.15 90)
		(size 2.2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "50" smd roundrect
		(at -5.5 20.15 90)
		(size 2.2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "51" smd roundrect
		(at -4.5 20.15 90)
		(size 2.2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "52" smd roundrect
		(at -3.5 20.15 90)
		(size 2.2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "53" smd roundrect
		(at -2.5 20.15 90)
		(size 2.2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "54" smd roundrect
		(at -1.5 20.15 90)
		(size 2.2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "55" smd roundrect
		(at -0.5 20.15 90)
		(size 2.2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "56" smd roundrect
		(at 0.5 20.15 90)
		(size 2.2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "57" smd roundrect
		(at 1.5 20.15 90)
		(size 2.2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "58" smd roundrect
		(at 2.5 20.15 90)
		(size 2.2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "59" smd roundrect
		(at 3.5 20.15 90)
		(size 2.2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "60" smd roundrect
		(at 4.5 20.15 90)
		(size 2.2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "61" smd roundrect
		(at 5.5 20.15 90)
		(size 2.2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "62" smd roundrect
		(at 6.5 20.15 90)
		(size 2.2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "63" smd roundrect
		(at 7.5 20.15 90)
		(size 2.2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "64" smd roundrect
		(at 8.5 20.15 90)
		(size 2.2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "65" smd roundrect
		(at 9.5 20.15 90)
		(size 2.2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "66" smd roundrect
		(at 10.5 20.15 90)
		(size 2.2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "67" smd roundrect
		(at 11.5 20.15 90)
		(size 2.2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "68" smd roundrect
		(at 12.5 20.15 90)
		(size 2.2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "69" smd roundrect
		(at 13.5 20.15 90)
		(size 2.2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "70" smd roundrect
		(at 14.5 20.15 90)
		(size 2.2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "71" smd roundrect
		(at 15.5 20.15 90)
		(size 2.2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "72" smd roundrect
		(at 16.5 20.15 90)
		(size 2.2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "73" smd roundrect
		(at 17.5 20.15 90)
		(size 2.2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "74" smd roundrect
		(at 20.15 18)
		(size 2.2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "75" smd roundrect
		(at 20.15 17)
		(size 2.2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "76" smd roundrect
		(at 20.15 16)
		(size 2.2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "77" smd roundrect
		(at 20.15 15)
		(size 2.2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "78" smd roundrect
		(at 20.15 14)
		(size 2.2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "79" smd roundrect
		(at 20.15 13)
		(size 2.2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "80" smd roundrect
		(at 20.15 12)
		(size 2.2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "81" smd roundrect
		(at 20.15 11)
		(size 2.2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "82" smd roundrect
		(at 20.15 10)
		(size 2.2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "83" smd roundrect
		(at 20.15 9)
		(size 2.2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "84" smd roundrect
		(at 20.15 8)
		(size 2.2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "85" smd roundrect
		(at 20.15 7)
		(size 2.2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "86" smd roundrect
		(at 20.15 6)
		(size 2.2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "87" smd roundrect
		(at 20.15 5)
		(size 2.2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "88" smd roundrect
		(at 20.15 4)
		(size 2.2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "89" smd roundrect
		(at 20.15 3)
		(size 2.2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "90" smd roundrect
		(at 20.15 2)
		(size 2.2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "91" smd roundrect
		(at 20.15 1)
		(size 2.2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "92" smd roundrect
		(at 20.15 0)
		(size 2.2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "93" smd roundrect
		(at 20.15 -1)
		(size 2.2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "94" smd roundrect
		(at 20.15 -2)
		(size 2.2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "95" smd roundrect
		(at 20.15 -3)
		(size 2.2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "96" smd roundrect
		(at 20.15 -4)
		(size 2.2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "97" smd roundrect
		(at 20.15 -5)
		(size 2.2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "98" smd roundrect
		(at 20.15 -6)
		(size 2.2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "99" smd roundrect
		(at 20.15 -7)
		(size 2.2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "100" smd roundrect
		(at 20.15 -8)
		(size 2.2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "101" smd roundrect
		(at 20.15 -9)
		(size 2.2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "102" smd roundrect
		(at 20.15 -10)
		(size 2.2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "103" smd roundrect
		(at 20.15 -11)
		(size 2.2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "104" smd roundrect
		(at 20.15 -12)
		(size 2.2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "105" smd roundrect
		(at 20.15 -13)
		(size 2.2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "106" smd roundrect
		(at 20.15 -14)
		(size 2.2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "107" smd roundrect
		(at 20.15 -15)
		(size 2.2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "108" smd roundrect
		(at 20.15 -16)
		(size 2.2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "109" smd roundrect
		(at 20.15 -17)
		(size 2.2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "110" smd roundrect
		(at 20.15 -18)
		(size 2.2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "111" smd roundrect
		(at 17.5 -20.15 90)
		(size 2.2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "112" smd roundrect
		(at 16.5 -20.15 90)
		(size 2.2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "113" smd roundrect
		(at 15.5 -20.15 90)
		(size 2.2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "114" smd roundrect
		(at 14.5 -20.15 90)
		(size 2.2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "115" smd roundrect
		(at 13.5 -20.15 90)
		(size 2.2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "116" smd roundrect
		(at 12.5 -20.15 90)
		(size 2.2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "117" smd roundrect
		(at 11.5 -20.15 90)
		(size 2.2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "118" smd roundrect
		(at 10.5 -20.15 90)
		(size 2.2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "119" smd roundrect
		(at 9.5 -20.15 90)
		(size 2.2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "120" smd roundrect
		(at 8.5 -20.15 90)
		(size 2.2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "121" smd roundrect
		(at 7.5 -20.15 90)
		(size 2.2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "122" smd roundrect
		(at 6.5 -20.15 90)
		(size 2.2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "123" smd roundrect
		(at 5.5 -20.15 90)
		(size 2.2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "124" smd roundrect
		(at 4.5 -20.15 90)
		(size 2.2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "125" smd roundrect
		(at 3.5 -20.15 90)
		(size 2.2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "126" smd roundrect
		(at 2.5 -20.15 90)
		(size 2.2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "127" smd roundrect
		(at 1.5 -20.15 90)
		(size 2.2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "128" smd roundrect
		(at 0.5 -20.15 90)
		(size 2.2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "129" smd roundrect
		(at -0.5 -20.15 90)
		(size 2.2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "130" smd roundrect
		(at -1.5 -20.15 90)
		(size 2.2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "131" smd roundrect
		(at -2.5 -20.15 90)
		(size 2.2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "132" smd roundrect
		(at -3.5 -20.15 90)
		(size 2.2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "133" smd roundrect
		(at -4.5 -20.15 90)
		(size 2.2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "134" smd roundrect
		(at -5.5 -20.15 90)
		(size 2.2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "135" smd roundrect
		(at -6.5 -20.15 90)
		(size 2.2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "136" smd roundrect
		(at -7.5 -20.15 90)
		(size 2.2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "137" smd roundrect
		(at -8.5 -20.15 90)
		(size 2.2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "138" smd roundrect
		(at -9.5 -20.15 90)
		(size 2.2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "139" smd roundrect
		(at -10.5 -20.15 90)
		(size 2.2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "140" smd roundrect
		(at -11.5 -20.15 90)
		(size 2.2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "141" smd roundrect
		(at -12.5 -20.15 90)
		(size 2.2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "142" smd roundrect
		(at -13.5 -20.15 90)
		(size 2.2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "143" smd roundrect
		(at -14.5 -20.15 90)
		(size 2.2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "144" smd roundrect
		(at -15.5 -20.15 90)
		(size 2.2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "145" smd roundrect
		(at -16.5 -20.15 90)
		(size 2.2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "146" smd roundrect
		(at -17.5 -20.15 90)
		(size 2.2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "147" smd roundrect
		(at -13.5 -10.5 90)
		(size 1.5 1.5)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.1666666667)
		(thermal_bridge_angle 45)
	)
	(pad "148" smd roundrect
		(at -13.5 -7.5 90)
		(size 1.5 1.5)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.1666666667)
		(thermal_bridge_angle 45)
	)
	(pad "149" smd roundrect
		(at -13.5 -4.5 90)
		(size 1.5 1.5)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.1666666667)
		(thermal_bridge_angle 45)
	)
	(pad "150" smd roundrect
		(at -13.5 -1.5 90)
		(size 1.5 1.5)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.1666666667)
		(thermal_bridge_angle 45)
	)
	(pad "151" smd roundrect
		(at -13.5 1.5 90)
		(size 1.5 1.5)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.1666666667)
		(thermal_bridge_angle 45)
	)
	(pad "152" smd roundrect
		(at -13.5 4.5 90)
		(size 1.5 1.5)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.1666666667)
		(thermal_bridge_angle 45)
	)
	(pad "153" smd roundrect
		(at -13.5 7.5 90)
		(size 1.5 1.5)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.1666666667)
		(thermal_bridge_angle 45)
	)
	(pad "154" smd roundrect
		(at -13.5 10.5 90)
		(size 1.5 1.5)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.1666666667)
		(thermal_bridge_angle 45)
	)
	(pad "155" smd roundrect
		(at -10.5 13.5 90)
		(size 1.5 1.5)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.1666666667)
		(thermal_bridge_angle 45)
	)
	(pad "156" smd roundrect
		(at -7.5 13.5 90)
		(size 1.5 1.5)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.1666666667)
		(thermal_bridge_angle 45)
	)
	(pad "157" smd roundrect
		(at -4.5 13.5 90)
		(size 1.5 1.5)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.1666666667)
		(thermal_bridge_angle 45)
	)
	(pad "158" smd roundrect
		(at -1.5 13.5 90)
		(size 1.5 1.5)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.1666666667)
		(thermal_bridge_angle 45)
	)
	(pad "159" smd roundrect
		(at 1.5 13.5 90)
		(size 1.5 1.5)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.1666666667)
		(thermal_bridge_angle 45)
	)
	(pad "160" smd roundrect
		(at 4.5 13.5 90)
		(size 1.5 1.5)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.1666666667)
		(thermal_bridge_angle 45)
	)
	(pad "161" smd roundrect
		(at 7.5 13.5 90)
		(size 1.5 1.5)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.1666666667)
		(thermal_bridge_angle 45)
	)
	(pad "162" smd roundrect
		(at 10.5 13.5 90)
		(size 1.5 1.5)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.1666666667)
		(thermal_bridge_angle 45)
	)
	(pad "163" smd roundrect
		(at 13.5 10.5 90)
		(size 1.5 1.5)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.1666666667)
		(thermal_bridge_angle 45)
	)
	(pad "164" smd roundrect
		(at 13.5 7.5 90)
		(size 1.5 1.5)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.1666666667)
		(thermal_bridge_angle 45)
	)
	(pad "165" smd roundrect
		(at 13.5 4.5 90)
		(size 1.5 1.5)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.1666666667)
		(thermal_bridge_angle 45)
	)
	(pad "166" smd roundrect
		(at 13.5 1.5 90)
		(size 1.5 1.5)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.1666666667)
		(thermal_bridge_angle 45)
	)
	(pad "167" smd roundrect
		(at 13.5 -1.5 90)
		(size 1.5 1.5)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.1666666667)
		(thermal_bridge_angle 45)
	)
	(pad "168" smd roundrect
		(at 13.5 -4.5 90)
		(size 1.5 1.5)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.1666666667)
		(thermal_bridge_angle 45)
	)
	(pad "169" smd roundrect
		(at 13.5 -7.5 90)
		(size 1.5 1.5)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.1666666667)
		(thermal_bridge_angle 45)
	)
	(pad "170" smd roundrect
		(at 13.5 -10.5 90)
		(size 1.5 1.5)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.1666666667)
		(thermal_bridge_angle 45)
	)
	(pad "171" smd roundrect
		(at 10.5 -13.5 90)
		(size 1.5 1.5)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.1666666667)
		(thermal_bridge_angle 45)
	)
	(pad "172" smd roundrect
		(at 7.5 -13.5 90)
		(size 1.5 1.5)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.1666666667)
		(thermal_bridge_angle 45)
	)
	(pad "173" smd roundrect
		(at 4.5 -13.5 90)
		(size 1.5 1.5)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.1666666667)
		(thermal_bridge_angle 45)
	)
	(pad "174" smd roundrect
		(at 1.5 -13.5 90)
		(size 1.5 1.5)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.1666666667)
		(thermal_bridge_angle 45)
	)
	(pad "175" smd roundrect
		(at -1.5 -13.5 90)
		(size 1.5 1.5)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.1666666667)
		(thermal_bridge_angle 45)
	)
	(pad "176" smd roundrect
		(at -4.5 -13.5 90)
		(size 1.5 1.5)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.1666666667)
		(thermal_bridge_angle 45)
	)
	(pad "177" smd roundrect
		(at -7.5 -13.5 90)
		(size 1.5 1.5)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.1666666667)
		(thermal_bridge_angle 45)
	)
	(pad "178" smd roundrect
		(at -10.5 -13.5 90)
		(size 1.5 1.5)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.1666666667)
		(thermal_bridge_angle 45)
	)
	(pad "179" smd roundrect
		(at -10.5 -4.5 90)
		(size 1.5 1.5)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.1666666667)
		(thermal_bridge_angle 45)
	)
	(pad "180" smd roundrect
		(at -10.5 -1.5 90)
		(size 1.5 1.5)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.1666666667)
		(thermal_bridge_angle 45)
	)
	(pad "181" smd roundrect
		(at -10.5 1.5 90)
		(size 1.5 1.5)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.1666666667)
		(thermal_bridge_angle 45)
	)
	(pad "182" smd roundrect
		(at -10.5 4.5 90)
		(size 1.5 1.5)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.1666666667)
		(thermal_bridge_angle 45)
	)
	(pad "183" smd roundrect
		(at -4.5 10.5 90)
		(size 1.5 1.5)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.1666666667)
		(thermal_bridge_angle 45)
	)
	(pad "184" smd roundrect
		(at -1.5 10.5 90)
		(size 1.5 1.5)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.1666666667)
		(thermal_bridge_angle 45)
	)
	(pad "185" smd roundrect
		(at 1.5 10.5 90)
		(size 1.5 1.5)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.1666666667)
		(thermal_bridge_angle 45)
	)
	(pad "186" smd roundrect
		(at 4.5 10.5 90)
		(size 1.5 1.5)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.1666666667)
		(thermal_bridge_angle 45)
	)
	(pad "187" smd roundrect
		(at 10.5 4.5 90)
		(size 1.5 1.5)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.1666666667)
		(thermal_bridge_angle 45)
	)
	(pad "188" smd roundrect
		(at 10.5 1.5 90)
		(size 1.5 1.5)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.1666666667)
		(thermal_bridge_angle 45)
	)
	(pad "189" smd roundrect
		(at 10.5 -1.5 90)
		(size 1.5 1.5)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.1666666667)
		(thermal_bridge_angle 45)
	)
	(pad "190" smd roundrect
		(at 10.5 -4.5 90)
		(size 1.5 1.5)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.1666666667)
		(thermal_bridge_angle 45)
	)
	(pad "191" smd roundrect
		(at 4.5 -10.5 90)
		(size 1.5 1.5)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.1666666667)
		(thermal_bridge_angle 45)
	)
	(pad "192" smd roundrect
		(at 1.5 -10.5 90)
		(size 1.5 1.5)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.1666666667)
		(thermal_bridge_angle 45)
	)
	(pad "193" smd roundrect
		(at -1.5 -10.5 90)
		(size 1.5 1.5)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.1666666667)
		(thermal_bridge_angle 45)
	)
	(pad "194" smd roundrect
		(at -4.5 -10.5 90)
		(size 1.5 1.5)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.1666666667)
		(thermal_bridge_angle 45)
	)
	(pad "195" smd roundrect
		(at -7.5 -4.5 90)
		(size 1.5 1.5)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.1666666667)
		(thermal_bridge_angle 45)
	)
	(pad "196" smd roundrect
		(at -7.5 -1.5 90)
		(size 1.5 1.5)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.1666666667)
		(thermal_bridge_angle 45)
	)
	(pad "197" smd roundrect
		(at -7.5 1.5 90)
		(size 1.5 1.5)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.1666666667)
		(thermal_bridge_angle 45)
	)
	(pad "198" smd roundrect
		(at -7.5 4.5 90)
		(size 1.5 1.5)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.1666666667)
		(thermal_bridge_angle 45)
	)
	(pad "199" smd roundrect
		(at -4.5 7.5 90)
		(size 1.5 1.5)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.1666666667)
		(thermal_bridge_angle 45)
	)
	(pad "200" smd roundrect
		(at -1.5 7.5 90)
		(size 1.5 1.5)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.1666666667)
		(thermal_bridge_angle 45)
	)
	(pad "201" smd roundrect
		(at 1.5 7.5 90)
		(size 1.5 1.5)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.1666666667)
		(thermal_bridge_angle 45)
	)
	(pad "202" smd roundrect
		(at 4.5 7.5 90)
		(size 1.5 1.5)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.1666666667)
		(thermal_bridge_angle 45)
	)
	(pad "203" smd roundrect
		(at 7.5 4.5 90)
		(size 1.5 1.5)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.1666666667)
		(thermal_bridge_angle 45)
	)
	(pad "204" smd roundrect
		(at 7.5 1.5 90)
		(size 1.5 1.5)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.1666666667)
		(thermal_bridge_angle 45)
	)
	(pad "205" smd roundrect
		(at 7.5 -1.5 90)
		(size 1.5 1.5)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.1666666667)
		(thermal_bridge_angle 45)
	)
	(pad "206" smd roundrect
		(at 7.5 -4.5 90)
		(size 1.5 1.5)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.1666666667)
		(thermal_bridge_angle 45)
	)
	(pad "207" smd roundrect
		(at 4.5 -7.5 90)
		(size 1.5 1.5)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.1666666667)
		(thermal_bridge_angle 45)
	)
	(pad "208" smd roundrect
		(at 1.5 -7.5 90)
		(size 1.5 1.5)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.1666666667)
		(thermal_bridge_angle 45)
	)
	(pad "209" smd roundrect
		(at -1.5 -7.5 90)
		(size 1.5 1.5)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.1666666667)
		(thermal_bridge_angle 45)
	)
	(pad "210" smd roundrect
		(at -4.5 -7.5 90)
		(size 1.5 1.5)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.1666666667)
		(thermal_bridge_angle 45)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F.Cu" "F.Fab")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy -0.68 -19.05) (xy -0.68 -16.65) (xy -4.33 -16.65) (xy -4.33 -19.05)
			)
		)
	)
	(embedded_fonts no)
	(model "${KICAD7_3DMODEL_DIR}/RF_GSM.3dshapes/Telit_SE150A4.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
