(footprint "Telit_xL865"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Telit xL865 familly footprint, http://www.telit.com/fileadmin/user_upload/products/Downloads/3G/Telit_UL865_Hardware_User_Guide_r8.pdf ")
	(tags "xL865 gsm umts")
	(property "Reference" "REF**"
		(at -13 -16 0)
		(layer "F.SilkS")
	)
	(property "Value" "Telit_xL865"
		(at 0 -3 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" smd circle
		(at -10 0 90)
		(size 2 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "" smd circle
		(at 0 -10 90)
		(size 2 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "" smd circle
		(at 0 10 90)
		(size 2 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "" smd circle
		(at 10 0 90)
		(size 2 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "1" smd oval
		(at -12 -9.8 90)
		(size 1 3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd oval
		(at -12 -8.3 90)
		(size 1 3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd oval
		(at -12 -6.8 90)
		(size 1 3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd oval
		(at -12 -5.3 90)
		(size 1 3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd oval
		(at -12 -3.8 90)
		(size 1 3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd oval
		(at -12 -2.3 90)
		(size 1 3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd oval
		(at -12 2.3 90)
		(size 1 3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd oval
		(at -12 3.8 90)
		(size 1 3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd oval
		(at -12 5.3 90)
		(size 1 3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd oval
		(at -12 6.8 90)
		(size 1 3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd oval
		(at -12 8.3 90)
		(size 1 3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "12" smd oval
		(at -12 9.8 90)
		(size 1 3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "13" smd oval
		(at -9.8 12)
		(size 1 3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "14" smd oval
		(at -8.3 12)
		(size 1 3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "15" smd oval
		(at -6.8 12)
		(size 1 3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "16" smd oval
		(at -5.3 12)
		(size 1 3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "17" smd oval
		(at -3.8 12)
		(size 1 3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "18" smd oval
		(at -2.3 12)
		(size 1 3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "19" smd oval
		(at 2.3 12)
		(size 1 3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "20" smd oval
		(at 3.8 12)
		(size 1 3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "21" smd oval
		(at 5.3 12)
		(size 1 3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "22" smd oval
		(at 6.8 12)
		(size 1 3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "23" smd oval
		(at 8.3 12)
		(size 1 3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "24" smd oval
		(at 9.8 12)
		(size 1 3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "25" smd oval
		(at 12 9.8 90)
		(size 1 3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "26" smd oval
		(at 12 8.3 90)
		(size 1 3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "27" smd oval
		(at 12 6.8 90)
		(size 1 3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "28" smd oval
		(at 12 5.3 90)
		(size 1 3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "29" smd oval
		(at 12 3.8 90)
		(size 1 3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "30" smd oval
		(at 12 2.3 90)
		(size 1 3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "31" smd oval
		(at 12 -2.3 90)
		(size 1 3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "32" smd oval
		(at 12 -3.8 90)
		(size 1 3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "33" smd oval
		(at 12 -5.3 90)
		(size 1 3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "34" smd oval
		(at 12 -6.8 90)
		(size 1 3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "35" smd oval
		(at 12 -8.3 90)
		(size 1 3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "36" smd oval
		(at 12 -9.8 90)
		(size 1 3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "37" smd oval
		(at 9.8 -12)
		(size 1 3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "38" smd oval
		(at 8.3 -12)
		(size 1 3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "39" smd oval
		(at 6.8 -12)
		(size 1 3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "40" smd oval
		(at 5.3 -12)
		(size 1 3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "41" smd oval
		(at 3.8 -12)
		(size 1 3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "42" smd oval
		(at 2.3 -12)
		(size 1 3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "43" smd oval
		(at -2.3 -12)
		(size 1 3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "44" smd oval
		(at -3.8 -12)
		(size 1 3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "45" smd oval
		(at -5.3 -12)
		(size 1 3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "46" smd oval
		(at -6.8 -12)
		(size 1 3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "47" smd oval
		(at -8.3 -12)
		(size 1 3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "48" smd oval
		(at -9.8 -12)
		(size 1 3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/RF_GSM.3dshapes/Telit_xL865.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
