(footprint "ublox_LENA-R8_LGA-100"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Multi-mode LTE Cat1 modules, https://content.u-blox.com/sites/default/files/documents/LENA-R8_SysIntegrManual_UBX-22015376.pdf#page=94 and https://content.u-blox.com/sites/default/files/documents/LENA-R8_DataSheet_UBX-22003110.pdf#page=35")
	(tags "ublox GSM LTE")
	(property "Reference" "REF**"
		(at 0 -16 0)
		(layer "F.SilkS")
	)
	(property "Value" "ublox_LENA-R8_LGA-100"
		(at 0 16.2 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(solder_mask_margin 0.05)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" smd roundrect
		(at -7 -11 270)
		(size 0.75 1.55)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at -7 -9.9 270)
		(size 0.75 1.55)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at -7 -8.8 270)
		(size 0.75 1.55)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at -7 -7.7 270)
		(size 0.75 1.55)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at -7 -6.6 270)
		(size 0.75 1.55)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at -7 -5.5 270)
		(size 0.75 1.55)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at -7 -4.4 270)
		(size 0.75 1.55)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at -7 -3.3 270)
		(size 0.75 1.55)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at -7 -2.2 270)
		(size 0.75 1.55)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at -7 -1.1 270)
		(size 0.75 1.55)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at -7 0 270)
		(size 0.75 1.55)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at -7 1.1 270)
		(size 0.75 1.55)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at -7 2.2 270)
		(size 0.75 1.55)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at -7 3.3 270)
		(size 0.75 1.55)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at -7 4.4 270)
		(size 0.75 1.55)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at -7 5.5 270)
		(size 0.75 1.55)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at -7 6.6 270)
		(size 0.75 1.55)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at -7 7.7 270)
		(size 0.75 1.55)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at -7 8.8 270)
		(size 0.75 1.55)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at -7 9.9 270)
		(size 0.75 1.55)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at -7 11 270)
		(size 0.75 1.55)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at -5.5 -12)
		(size 0.75 1.55)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at -5.5 12)
		(size 0.75 1.55)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at -5.25 -10.25 180)
		(size 1.05 1.05)
		(layers "F.Paste")
		(roundrect_rratio 0.2380952381)
	)
	(pad "" smd roundrect
		(at -5.25 -8.45 180)
		(size 1.05 1.05)
		(layers "F.Paste")
		(roundrect_rratio 0.2380952381)
	)
	(pad "" smd roundrect
		(at -5.25 -6.65 180)
		(size 1.05 1.05)
		(layers "F.Paste")
		(roundrect_rratio 0.2380952381)
	)
	(pad "" smd roundrect
		(at -5.25 -3.05 180)
		(size 1.05 1.05)
		(layers "F.Paste")
		(roundrect_rratio 0.2380952381)
	)
	(pad "" smd roundrect
		(at -5.25 3.05 180)
		(size 1.05 1.05)
		(layers "F.Paste")
		(roundrect_rratio 0.2380952381)
	)
	(pad "" smd roundrect
		(at -5.25 6.65 180)
		(size 1.05 1.05)
		(layers "F.Paste")
		(roundrect_rratio 0.2380952381)
	)
	(pad "" smd roundrect
		(at -5.25 8.45 180)
		(size 1.05 1.05)
		(layers "F.Paste")
		(roundrect_rratio 0.2380952381)
	)
	(pad "" smd roundrect
		(at -5.25 10.25 180)
		(size 1.05 1.05)
		(layers "F.Paste")
		(roundrect_rratio 0.2380952381)
	)
	(pad "" smd roundrect
		(at -4.4 -12)
		(size 0.75 1.55)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at -4.4 12)
		(size 0.75 1.55)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at -3.3 -12)
		(size 0.75 1.55)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at -3.3 12)
		(size 0.75 1.55)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at -3.15 -10.25 180)
		(size 1.05 1.05)
		(layers "F.Paste")
		(roundrect_rratio 0.2380952381)
	)
	(pad "" smd roundrect
		(at -3.15 -8.45 180)
		(size 1.05 1.05)
		(layers "F.Paste")
		(roundrect_rratio 0.2380952381)
	)
	(pad "" smd roundrect
		(at -3.15 8.45 180)
		(size 1.05 1.05)
		(layers "F.Paste")
		(roundrect_rratio 0.2380952381)
	)
	(pad "" smd roundrect
		(at -3.15 10.25 180)
		(size 1.05 1.05)
		(layers "F.Paste")
		(roundrect_rratio 0.2380952381)
	)
	(pad "" smd roundrect
		(at -2.2 -12)
		(size 0.75 1.55)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at -2.2 12)
		(size 0.75 1.55)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at -1.1 -12)
		(size 0.75 1.55)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at -1.1 12)
		(size 0.75 1.55)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at -1.05 -10.25 180)
		(size 1.05 1.05)
		(layers "F.Paste")
		(roundrect_rratio 0.2380952381)
	)
	(pad "" smd roundrect
		(at -1.05 -8.45 180)
		(size 1.05 1.05)
		(layers "F.Paste")
		(roundrect_rratio 0.2380952381)
	)
	(pad "" smd roundrect
		(at -1.05 -6.65 180)
		(size 1.05 1.05)
		(layers "F.Paste")
		(roundrect_rratio 0.2380952381)
	)
	(pad "" smd roundrect
		(at -1.05 6.65 180)
		(size 1.05 1.05)
		(layers "F.Paste")
		(roundrect_rratio 0.2380952381)
	)
	(pad "" smd roundrect
		(at -1.05 8.45 180)
		(size 1.05 1.05)
		(layers "F.Paste")
		(roundrect_rratio 0.2380952381)
	)
	(pad "" smd roundrect
		(at -1.05 10.25 180)
		(size 1.05 1.05)
		(layers "F.Paste")
		(roundrect_rratio 0.2380952381)
	)
	(pad "" smd roundrect
		(at 0 -12)
		(size 0.75 1.55)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 0 12)
		(size 0.75 1.55)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 1.05 -10.25 180)
		(size 1.05 1.05)
		(layers "F.Paste")
		(roundrect_rratio 0.2380952381)
	)
	(pad "" smd roundrect
		(at 1.05 -8.45 180)
		(size 1.05 1.05)
		(layers "F.Paste")
		(roundrect_rratio 0.2380952381)
	)
	(pad "" smd roundrect
		(at 1.05 -6.65 180)
		(size 1.05 1.05)
		(layers "F.Paste")
		(roundrect_rratio 0.2380952381)
	)
	(pad "" smd roundrect
		(at 1.05 6.65 180)
		(size 1.05 1.05)
		(layers "F.Paste")
		(roundrect_rratio 0.2380952381)
	)
	(pad "" smd roundrect
		(at 1.05 8.45 180)
		(size 1.05 1.05)
		(layers "F.Paste")
		(roundrect_rratio 0.2380952381)
	)
	(pad "" smd roundrect
		(at 1.05 10.25 180)
		(size 1.05 1.05)
		(layers "F.Paste")
		(roundrect_rratio 0.2380952381)
	)
	(pad "" smd roundrect
		(at 1.1 -12)
		(size 0.75 1.55)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 1.1 12)
		(size 0.75 1.55)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 2.2 -12)
		(size 0.75 1.55)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 2.2 12)
		(size 0.75 1.55)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 3.15 -10.25 180)
		(size 1.05 1.05)
		(layers "F.Paste")
		(roundrect_rratio 0.2380952381)
	)
	(pad "" smd roundrect
		(at 3.15 -8.45 180)
		(size 1.05 1.05)
		(layers "F.Paste")
		(roundrect_rratio 0.2380952381)
	)
	(pad "" smd roundrect
		(at 3.15 8.45 180)
		(size 1.05 1.05)
		(layers "F.Paste")
		(roundrect_rratio 0.2380952381)
	)
	(pad "" smd roundrect
		(at 3.15 10.25 180)
		(size 1.05 1.05)
		(layers "F.Paste")
		(roundrect_rratio 0.2380952381)
	)
	(pad "" smd roundrect
		(at 3.3 -12)
		(size 0.75 1.55)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 3.3 12)
		(size 0.75 1.55)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 4.4 -12)
		(size 0.75 1.55)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 4.4 12)
		(size 0.75 1.55)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 5.25 -10.25 180)
		(size 1.05 1.05)
		(layers "F.Paste")
		(roundrect_rratio 0.2380952381)
	)
	(pad "" smd roundrect
		(at 5.25 -8.45 180)
		(size 1.05 1.05)
		(layers "F.Paste")
		(roundrect_rratio 0.2380952381)
	)
	(pad "" smd roundrect
		(at 5.25 -6.65 180)
		(size 1.05 1.05)
		(layers "F.Paste")
		(roundrect_rratio 0.2380952381)
	)
	(pad "" smd roundrect
		(at 5.25 -3.05 180)
		(size 1.05 1.05)
		(layers "F.Paste")
		(roundrect_rratio 0.2380952381)
	)
	(pad "" smd roundrect
		(at 5.25 3.05 180)
		(size 1.05 1.05)
		(layers "F.Paste")
		(roundrect_rratio 0.2380952381)
	)
	(pad "" smd roundrect
		(at 5.25 6.65 180)
		(size 1.05 1.05)
		(layers "F.Paste")
		(roundrect_rratio 0.2380952381)
	)
	(pad "" smd roundrect
		(at 5.25 8.45 180)
		(size 1.05 1.05)
		(layers "F.Paste")
		(roundrect_rratio 0.2380952381)
	)
	(pad "" smd roundrect
		(at 5.25 10.25 180)
		(size 1.05 1.05)
		(layers "F.Paste")
		(roundrect_rratio 0.2380952381)
	)
	(pad "" smd roundrect
		(at 5.5 -12)
		(size 0.75 1.55)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 5.5 12)
		(size 0.75 1.55)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 7 -11 270)
		(size 0.75 1.55)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 7 -9.9 270)
		(size 0.75 1.55)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 7 -8.8 270)
		(size 0.75 1.55)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 7 -7.7 270)
		(size 0.75 1.55)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 7 -6.6 270)
		(size 0.75 1.55)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 7 -5.5 270)
		(size 0.75 1.55)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 7 -4.4 270)
		(size 0.75 1.55)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 7 -3.3 270)
		(size 0.75 1.55)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 7 -2.2 270)
		(size 0.75 1.55)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 7 -1.1 270)
		(size 0.75 1.55)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 7 0 270)
		(size 0.75 1.55)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 7 1.1 270)
		(size 0.75 1.55)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 7 2.2 270)
		(size 0.75 1.55)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 7 3.3 270)
		(size 0.75 1.55)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 7 4.4 270)
		(size 0.75 1.55)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 7 5.5 270)
		(size 0.75 1.55)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 7 6.6 270)
		(size 0.75 1.55)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 7 7.7 270)
		(size 0.75 1.55)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 7 8.8 270)
		(size 0.75 1.55)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 7 9.9 270)
		(size 0.75 1.55)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 7 11 270)
		(size 0.75 1.55)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "1" smd rect
		(at -6.95 -11 270)
		(size 0.8 1.5)
		(layers "F.Cu" "F.Mask")
	)
	(pad "2" smd rect
		(at -6.95 -9.9 270)
		(size 0.8 1.5)
		(layers "F.Cu" "F.Mask")
	)
	(pad "3" smd rect
		(at -6.95 -8.8 270)
		(size 0.8 1.5)
		(layers "F.Cu" "F.Mask")
	)
	(pad "4" smd rect
		(at -6.95 -7.7 270)
		(size 0.8 1.5)
		(layers "F.Cu" "F.Mask")
	)
	(pad "5" smd rect
		(at -6.95 -6.6 270)
		(size 0.8 1.5)
		(layers "F.Cu" "F.Mask")
	)
	(pad "6" smd rect
		(at -6.95 -5.5 270)
		(size 0.8 1.5)
		(layers "F.Cu" "F.Mask")
	)
	(pad "7" smd rect
		(at -6.95 -4.4 270)
		(size 0.8 1.5)
		(layers "F.Cu" "F.Mask")
	)
	(pad "8" smd rect
		(at -6.95 -3.3 270)
		(size 0.8 1.5)
		(layers "F.Cu" "F.Mask")
	)
	(pad "9" smd rect
		(at -6.95 -2.2 270)
		(size 0.8 1.5)
		(layers "F.Cu" "F.Mask")
	)
	(pad "10" smd rect
		(at -6.95 -1.1 270)
		(size 0.8 1.5)
		(layers "F.Cu" "F.Mask")
	)
	(pad "11" smd rect
		(at -6.95 0 270)
		(size 0.8 1.5)
		(layers "F.Cu" "F.Mask")
	)
	(pad "12" smd rect
		(at -6.95 1.1 270)
		(size 0.8 1.5)
		(layers "F.Cu" "F.Mask")
	)
	(pad "13" smd rect
		(at -6.95 2.2 270)
		(size 0.8 1.5)
		(layers "F.Cu" "F.Mask")
	)
	(pad "14" smd rect
		(at -6.95 3.3 270)
		(size 0.8 1.5)
		(layers "F.Cu" "F.Mask")
	)
	(pad "15" smd rect
		(at -6.95 4.4 270)
		(size 0.8 1.5)
		(layers "F.Cu" "F.Mask")
	)
	(pad "16" smd rect
		(at -6.95 5.5 270)
		(size 0.8 1.5)
		(layers "F.Cu" "F.Mask")
	)
	(pad "17" smd rect
		(at -6.95 6.6 270)
		(size 0.8 1.5)
		(layers "F.Cu" "F.Mask")
	)
	(pad "18" smd rect
		(at -6.95 7.7 270)
		(size 0.8 1.5)
		(layers "F.Cu" "F.Mask")
	)
	(pad "19" smd rect
		(at -6.95 8.8 270)
		(size 0.8 1.5)
		(layers "F.Cu" "F.Mask")
	)
	(pad "20" smd rect
		(at -6.95 9.9 270)
		(size 0.8 1.5)
		(layers "F.Cu" "F.Mask")
	)
	(pad "21" smd rect
		(at -6.95 11 270)
		(size 0.8 1.5)
		(layers "F.Cu" "F.Mask")
	)
	(pad "22" smd rect
		(at -5.5 11.95)
		(size 0.8 1.5)
		(layers "F.Cu" "F.Mask")
	)
	(pad "23" smd rect
		(at -4.4 11.95)
		(size 0.8 1.5)
		(layers "F.Cu" "F.Mask")
	)
	(pad "24" smd rect
		(at -3.3 11.95)
		(size 0.8 1.5)
		(layers "F.Cu" "F.Mask")
	)
	(pad "25" smd rect
		(at -2.2 11.95)
		(size 0.8 1.5)
		(layers "F.Cu" "F.Mask")
	)
	(pad "26" smd rect
		(at -1.1 11.95)
		(size 0.8 1.5)
		(layers "F.Cu" "F.Mask")
	)
	(pad "27" smd rect
		(at 0 11.95)
		(size 0.8 1.5)
		(layers "F.Cu" "F.Mask")
	)
	(pad "28" smd rect
		(at 1.1 11.95)
		(size 0.8 1.5)
		(layers "F.Cu" "F.Mask")
	)
	(pad "29" smd rect
		(at 2.2 11.95)
		(size 0.8 1.5)
		(layers "F.Cu" "F.Mask")
	)
	(pad "30" smd rect
		(at 3.3 11.95)
		(size 0.8 1.5)
		(layers "F.Cu" "F.Mask")
	)
	(pad "31" smd rect
		(at 4.4 11.95)
		(size 0.8 1.5)
		(layers "F.Cu" "F.Mask")
	)
	(pad "32" smd rect
		(at 5.5 11.95)
		(size 0.8 1.5)
		(layers "F.Cu" "F.Mask")
	)
	(pad "33" smd rect
		(at 6.95 11 90)
		(size 0.8 1.5)
		(layers "F.Cu" "F.Mask")
	)
	(pad "34" smd rect
		(at 6.95 9.9 90)
		(size 0.8 1.5)
		(layers "F.Cu" "F.Mask")
	)
	(pad "35" smd rect
		(at 6.95 8.8 90)
		(size 0.8 1.5)
		(layers "F.Cu" "F.Mask")
	)
	(pad "36" smd rect
		(at 6.95 7.7 90)
		(size 0.8 1.5)
		(layers "F.Cu" "F.Mask")
	)
	(pad "37" smd rect
		(at 6.95 6.6 90)
		(size 0.8 1.5)
		(layers "F.Cu" "F.Mask")
	)
	(pad "38" smd rect
		(at 6.95 5.5 90)
		(size 0.8 1.5)
		(layers "F.Cu" "F.Mask")
	)
	(pad "39" smd rect
		(at 6.95 4.4 90)
		(size 0.8 1.5)
		(layers "F.Cu" "F.Mask")
	)
	(pad "40" smd rect
		(at 6.95 3.3 90)
		(size 0.8 1.5)
		(layers "F.Cu" "F.Mask")
	)
	(pad "41" smd rect
		(at 6.95 2.2 90)
		(size 0.8 1.5)
		(layers "F.Cu" "F.Mask")
	)
	(pad "42" smd rect
		(at 6.95 1.1 90)
		(size 0.8 1.5)
		(layers "F.Cu" "F.Mask")
	)
	(pad "43" smd rect
		(at 6.95 0 90)
		(size 0.8 1.5)
		(layers "F.Cu" "F.Mask")
	)
	(pad "44" smd rect
		(at 6.95 -1.1 90)
		(size 0.8 1.5)
		(layers "F.Cu" "F.Mask")
	)
	(pad "45" smd rect
		(at 6.95 -2.2 90)
		(size 0.8 1.5)
		(layers "F.Cu" "F.Mask")
	)
	(pad "46" smd rect
		(at 6.95 -3.3 90)
		(size 0.8 1.5)
		(layers "F.Cu" "F.Mask")
	)
	(pad "47" smd rect
		(at 6.95 -4.4 90)
		(size 0.8 1.5)
		(layers "F.Cu" "F.Mask")
	)
	(pad "48" smd rect
		(at 6.95 -5.5 90)
		(size 0.8 1.5)
		(layers "F.Cu" "F.Mask")
	)
	(pad "49" smd rect
		(at 6.95 -6.6 90)
		(size 0.8 1.5)
		(layers "F.Cu" "F.Mask")
	)
	(pad "50" smd rect
		(at 6.95 -7.7 90)
		(size 0.8 1.5)
		(layers "F.Cu" "F.Mask")
	)
	(pad "51" smd rect
		(at 6.95 -8.8 90)
		(size 0.8 1.5)
		(layers "F.Cu" "F.Mask")
	)
	(pad "52" smd rect
		(at 6.95 -9.9 90)
		(size 0.8 1.5)
		(layers "F.Cu" "F.Mask")
	)
	(pad "53" smd rect
		(at 6.95 -11 90)
		(size 0.8 1.5)
		(layers "F.Cu" "F.Mask")
	)
	(pad "54" smd rect
		(at 5.5 -11.95 180)
		(size 0.8 1.5)
		(layers "F.Cu" "F.Mask")
	)
	(pad "55" smd rect
		(at 4.4 -11.95 180)
		(size 0.8 1.5)
		(layers "F.Cu" "F.Mask")
	)
	(pad "56" smd rect
		(at 3.3 -11.95 180)
		(size 0.8 1.5)
		(layers "F.Cu" "F.Mask")
	)
	(pad "57" smd rect
		(at 2.2 -11.95 180)
		(size 0.8 1.5)
		(layers "F.Cu" "F.Mask")
	)
	(pad "58" smd rect
		(at 1.1 -11.95 180)
		(size 0.8 1.5)
		(layers "F.Cu" "F.Mask")
	)
	(pad "59" smd rect
		(at 0 -11.95 180)
		(size 0.8 1.5)
		(layers "F.Cu" "F.Mask")
	)
	(pad "60" smd rect
		(at -1.1 -11.95 180)
		(size 0.8 1.5)
		(layers "F.Cu" "F.Mask")
	)
	(pad "61" smd rect
		(at -2.2 -11.95 180)
		(size 0.8 1.5)
		(layers "F.Cu" "F.Mask")
	)
	(pad "62" smd rect
		(at -3.3 -11.95 180)
		(size 0.8 1.5)
		(layers "F.Cu" "F.Mask")
	)
	(pad "63" smd rect
		(at -4.4 -11.95 180)
		(size 0.8 1.5)
		(layers "F.Cu" "F.Mask")
	)
	(pad "64" smd rect
		(at -5.5 -11.95 180)
		(size 0.8 1.5)
		(layers "F.Cu" "F.Mask")
	)
	(pad "65" smd rect
		(at -5.25 -10.25 180)
		(size 1.1 1.1)
		(layers "F.Cu" "F.Mask")
	)
	(pad "66" smd rect
		(at -3.15 -10.25 180)
		(size 1.1 1.1)
		(layers "F.Cu" "F.Mask")
	)
	(pad "67" smd rect
		(at -1.05 -10.25 180)
		(size 1.1 1.1)
		(layers "F.Cu" "F.Mask")
	)
	(pad "68" smd rect
		(at 1.05 -10.25 180)
		(size 1.1 1.1)
		(layers "F.Cu" "F.Mask")
	)
	(pad "69" smd rect
		(at 3.15 -10.25 180)
		(size 1.1 1.1)
		(layers "F.Cu" "F.Mask")
	)
	(pad "70" smd rect
		(at 5.25 -10.25 180)
		(size 1.1 1.1)
		(layers "F.Cu" "F.Mask")
	)
	(pad "71" smd rect
		(at -5.25 -8.45 180)
		(size 1.1 1.1)
		(layers "F.Cu" "F.Mask")
	)
	(pad "72" smd rect
		(at -3.15 -8.45 180)
		(size 1.1 1.1)
		(layers "F.Cu" "F.Mask")
	)
	(pad "73" smd rect
		(at -1.05 -8.45 180)
		(size 1.1 1.1)
		(layers "F.Cu" "F.Mask")
	)
	(pad "74" smd rect
		(at 1.05 -8.45 180)
		(size 1.1 1.1)
		(layers "F.Cu" "F.Mask")
	)
	(pad "75" smd rect
		(at 3.15 -8.45 180)
		(size 1.1 1.1)
		(layers "F.Cu" "F.Mask")
	)
	(pad "76" smd rect
		(at 5.25 -8.45 180)
		(size 1.1 1.1)
		(layers "F.Cu" "F.Mask")
	)
	(pad "77" smd rect
		(at -5.25 -6.65 180)
		(size 1.1 1.1)
		(layers "F.Cu" "F.Mask")
	)
	(pad "78" smd rect
		(at 5.25 -6.65 180)
		(size 1.1 1.1)
		(layers "F.Cu" "F.Mask")
	)
	(pad "79" smd rect
		(at -5.25 -3.05 180)
		(size 1.1 1.1)
		(layers "F.Cu" "F.Mask")
	)
	(pad "80" smd rect
		(at 5.25 -3.05 180)
		(size 1.1 1.1)
		(layers "F.Cu" "F.Mask")
	)
	(pad "81" smd rect
		(at -5.25 3.05 180)
		(size 1.1 1.1)
		(layers "F.Cu" "F.Mask")
	)
	(pad "82" smd rect
		(at 5.25 3.05 180)
		(size 1.1 1.1)
		(layers "F.Cu" "F.Mask")
	)
	(pad "83" smd rect
		(at -5.25 6.65 180)
		(size 1.1 1.1)
		(layers "F.Cu" "F.Mask")
	)
	(pad "84" smd rect
		(at 5.25 6.65 180)
		(size 1.1 1.1)
		(layers "F.Cu" "F.Mask")
	)
	(pad "85" smd rect
		(at -5.25 8.45 180)
		(size 1.1 1.1)
		(layers "F.Cu" "F.Mask")
	)
	(pad "86" smd rect
		(at -3.15 8.45 180)
		(size 1.1 1.1)
		(layers "F.Cu" "F.Mask")
	)
	(pad "87" smd rect
		(at -1.05 8.45 180)
		(size 1.1 1.1)
		(layers "F.Cu" "F.Mask")
	)
	(pad "88" smd rect
		(at 1.05 8.45 180)
		(size 1.1 1.1)
		(layers "F.Cu" "F.Mask")
	)
	(pad "89" smd rect
		(at 3.15 8.45 180)
		(size 1.1 1.1)
		(layers "F.Cu" "F.Mask")
	)
	(pad "90" smd rect
		(at 5.25 8.45 180)
		(size 1.1 1.1)
		(layers "F.Cu" "F.Mask")
	)
	(pad "91" smd rect
		(at -5.25 10.25 180)
		(size 1.1 1.1)
		(layers "F.Cu" "F.Mask")
	)
	(pad "92" smd rect
		(at -3.15 10.25 180)
		(size 1.1 1.1)
		(layers "F.Cu" "F.Mask")
	)
	(pad "93" smd rect
		(at -1.05 10.25 270)
		(size 1.1 1.1)
		(layers "F.Cu" "F.Mask")
	)
	(pad "94" smd rect
		(at 1.05 10.25 180)
		(size 1.1 1.1)
		(layers "F.Cu" "F.Mask")
	)
	(pad "95" smd rect
		(at 3.15 10.25 180)
		(size 1.1 1.1)
		(layers "F.Cu" "F.Mask")
	)
	(pad "96" smd rect
		(at 5.25 10.25 270)
		(size 1.1 1.1)
		(layers "F.Cu" "F.Mask")
	)
	(pad "97" smd rect
		(at -1.05 -6.65 180)
		(size 1.1 1.1)
		(layers "F.Cu" "F.Mask")
	)
	(pad "98" smd rect
		(at 1.05 -6.65 180)
		(size 1.1 1.1)
		(layers "F.Cu" "F.Mask")
	)
	(pad "99" smd rect
		(at -1.05 6.65 180)
		(size 1.1 1.1)
		(layers "F.Cu" "F.Mask")
	)
	(pad "100" smd rect
		(at 1.05 6.65 180)
		(size 1.1 1.1)
		(layers "F.Cu" "F.Mask")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/RF_GSM.3dshapes/ublox_LENA-R8_LGA-100.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
